{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":12,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYA-DV3P-H-"]
[]
[]
[]
[]
["","","","","","EWYA004D2V3P-H","EWYA006D2V3P-H","EWYA008D2V3P-H","EWYA009DAV3P-H-","EWYA011DAV3P-H-","EWYA014DAV3P-H-","EWYA016DAV3P-H-"]
["Koelcapaciteit","Nom.","","","kW","4.86 (1), 4.52 (2)","5.83 (1), 5.09 (2)","6.18 (1), 5.44 (2)","9.35 (1), 9.10 (2)","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Capaciteitsregeling","Methode","","","","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.820 (1), 1.36 (2)","1.08 (1), 1.55 (2)","1.19 (1), 1.73 (2)","2.79 (1), 1.71 (2)","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["EER","","","","","5.91 (1), 3.32 (2)","5.40 (1), 3.28 (2)","5.19 (1), 3.14 (2)","3.35 (1), 5.34 (2)","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["SEER","","","","","","","","5.62 (5)","5.79 (5)","5.71 (5)","5.59 (5)"]
["Afmetingen","Unit","","Diepte","mm","362","362","362","460","460","460","460"]
["","","","Hoogte","mm","770","770","770","870","870","870","870"]
["","","","Breedte","mm","1250","1250","1250","1380","1380","1380","1380"]
["Gewicht","Unit","","","kg","88","88","88","147","147","147","147"]
["Behuizing","Kleur","","","","Ivoorwit","Ivoorwit","Ivoorwit","Ivoorwit","Ivoorwit","Ivoorwit","Ivoorwit"]
["","Materiaal","","","","Verzinkt plaatstaal","Verzinkt plaatstaal","Verzinkt plaatstaal","Gegalvaniseerde staalplaat met polyesterlak","Gegalvaniseerde staalplaat met polyesterlak","Gegalvaniseerde staalplaat met polyesterlak","Gegalvaniseerde staalplaat met polyesterlak"]
["Luchtwarmtewisselaar","Type","","","","","","","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler"]
["Ventilator","Aantal","","","","1","1","1","1","1","1","1"]
["","Type","","","","Schroefventilator","Schroefventilator","Schroefventilator","Schroefventilator","Schroefventilator","Schroefventilator","Schroefventilator"]
["Ventilatormotor","Aandrijving","","","","","","","Directe aandrijving","Directe aandrijving","Directe aandrijving","Directe aandrijving"]
["Compressor","Hoeveelheid","","","","1","1","1","1","1","1","1"]
["","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor"]
["","Aanloopmethode_","","","","","","","Invertergestuurd","Invertergestuurd","Invertergestuurd","Invertergestuurd"]
["Werkbereik","Luchtzijde","Koelen","Min.","°CDB","10 (3)","10 (3)","10 (3)","10","10","10","10"]
["","","","Max.","°CDB","43","43","43","43","43","43","43"]
["Bedrijfsbereik","Waterkant","Verdamper","Min.","°CDB","5 (3)","5 (3)","5 (3)","5","5","5","5"]
["","","","Max.","°CDB","22","22","22","22","22","22","22"]
["Geluidsvermogenniveau","Koelen","","Nom.","dBA","61","62","62","65.5","67.0","69.0","69.0"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","48","49","50","44.0","47.7","50.8","51.0"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675","675","675.0","675.0","675.0","675.0"]
["","Vulling","","","kg","1.35","1.35","1.35"]
["Koudemiddel","Circuits","","Aantal","","","","","1","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50","50","50","50"]
["","Spanning","","","V","230 +/-10%","230 +/-10%","230 +/-10%","230","230","230","230"]
["","Spanningsbereik","","Min.","%","","","","-10","-10","-10","-10"]
["","","","Spanningsvoeding-=-Spanningsbereik-=-Max.-=-%","%","","","","10","10","10","10"]
["Unit","Bedrijfsstroom","","Max.","A","","","","30.8","30.8","30.8","30.8"]
["Opmerkingen","","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB"]
["","","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(3) - Raadpleeg de werkbereik-tekening voor meer informatie","(3) - Raadpleeg de werkbereik-tekening voor meer informatie","(3) - Raadpleeg de werkbereik-tekening voor meer informatie","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","","","","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","","","","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825"]
["","","","","","","","","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding"]
["","","","","","","","","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie"]