{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["","","Middelhoog","dBA","42","45"]
["","","Laag","dBA","40","41"]
["","Koelen","Middelhoog","dBA","42","45"]
["","","Laag","dBA","40","41"]
["","","Hoog","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["Koelcapaciteit","Totale capaciteit","Nom.","kW","0.051","0.061"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","9.52","9.52"]
["","Gas","Buitendiameter","mm","15.9","15.9"]
["","Drainage","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Sound power level","Koelen","","dBA","61","65"]
["","Verwarmen","","dBA","61","65"]
["Afmetingen","Unit","Breedte","mm","1,050","1,200"]
["","","Diepte","mm","238","240"]
["","","Hoogte","mm","290","340"]
["Casing","Material","","","Hars","Hars"]
["","Colour","","","Zuiver wit","Zuiver wit"]
["Gewicht","Unit","","kg","13","17"]
["Verwarmingscapaciteit","Totaalvermogen","Nom.","kW","0.068","0.061"]
["Power supply","Phase","","","1~","1~"]
["","Frequentie","","Hz","50","50"]
["","Spanning","","V","220-240","220-240"]