{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / AZAS-MY"]
[]
[]
[]
[]
["","","","","FBA100A2VEB / AZAS100MUY","FBA125A2VEB / AZAS125MUY","FBA140A2VEB / AZAS140MUY"]
["Totale koelcapaciteit","Totale koelcapaciteit-=-Nom.-=-kW","","kW","","12.1 (1)","13.4 (1)"]
["Totale verwarmingscapaciteit","Totale verwarmingscapaciteit-=-Nom.-=-kW","","kW","","13.5 (2)","15.5 (2)"]
["Koeling","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","9.5","12.1","13.4"]
["","SEER","","","5.67","5.24","5.72"]
["","Jaarlijks energieverbruik","","kWu/a","586","1385","1406"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A"]
["","Vermogen","Pdesign","kW","6","6","7.8"]
["","SCOP/A","","","3.81","3.55","3.85"]
["","Jaarlijks energieverbruik","","kWu/a","2205","2366","2836"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Koelcapaciteit","Nom.","","kW","9.5"]
["Verwarmingscapaciteit","Nom.","","kW","10.8 (2)"]