{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXS-L"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXS50L2V1B","FBA60A2VEB9 / RXS60L2V1B"]
["Koelcapaciteit","Nom.","","kW","","5.70"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","","826"]
["","EER","","","","3.45"]
["","COP","","","","37.10"]
["","Richtlijn Energielabels","Koeling","","","A"]
["","","Verwarming","","","A"]
["Verwarmingscapaciteit","Nom.","","kW","","7.00"]
["Opmerkingen","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Buitenunit","","","","RXS50L2V1B"]
["Koelcapaciteit","Nom.","","kW","5.00"]
["Verwarmingscapaciteit","Nom.","","kW","5.50"]
["Nominaal rendement","EER","","","3.52"]
["","COP","","","38.30"]
["","Jaarlijks energieverbruik","","kWh","710"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","A"]
["Koeling","Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","5.00"]
["","SEER","","","6.21"]
["","Jaarlijks energieverbruik","","kWu/a","282"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","4.40"]
["","SCOP/A","","","4.06"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.73"]
["","Jaarlijks energieverbruik","","kWu/a","1517"]
["Bereik van het energierendement","","","","A+++ ~ D"]