{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZAG-B"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / RZAG35B5V1B","FBA50A2VEB9 / RZAG35B5V1B","FBA60A2VEB9 / RZAG50B5V1B","FBA50A2VEB9 / RZAG50B5V1B","FBA60A2VEB9 / RZAG60B5V1B","FBA71A2VEB9 / RZAG60B5V1B"]
["Koelcapaciteit","Min.","","kW","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","5","5","6","6"]
["","Max.","","kW","5","5","6","6","7","7"]
["Verwarmingscapaciteit","Min.","","kW","1.4","1.4","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","4","4","6","6","7","7"]
["","Max.","","kW","5","5","6","6","7.5","7.5"]
["Nominaal rendement","EER","","","4.5","4.62","4.11","4","4.05","4.31"]
["","COP","","","4.4","4.44","3.97","3.8","3.8","3.87"]
["","Jaarlijks energieverbruik","","kWh","389","379","608","625","741","696"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A","A","A","A","A"]
["","","Verwarming","","A","A","A","A","C","A"]
["Koeling","Energieklasse","","","A++","A++","A++","A++","A++","A++"]
["","Vermogen","Pdesign","kW","3.5","3.5","5","5","6","6"]
["","SEER","","","6.12","6.17","6.63","6.3","6.15","6.25"]
["","Jaarlijks energieverbruik","","kWu/a","200","199","264","278","341","336"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+","A+","A+","A+","A+","A+"]
["","Vermogen","Pdesign","kW","4.2","4.2","4.3","4.3","4.5","4.5"]
["","SCOP/A","","","4.1","4.14","4.28","4.1","4.1","4.18"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.49","3.51","3.75","3.65","3.85","3.86"]
["","Jaarlijks energieverbruik","","kWu/a","1434","1420","1406","1469","1537","1508"]