{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":12,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9)"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB9","FBA50A2VEB9","FBA60A2VEB9","FBA71A2VEB9","FBA100A2VEB","FBA125A2VEB","FBA140A2VEB"]
["Koelcapaciteit","Koelcapaciteit-=-Totale capaciteit","","Koelcapaciteit-=-Totale capaciteit-=-Nom.-=-kW","kW","","","","","","14.00","15.40"]
["Verwarmingscapaciteit","Verwarmingscapaciteit-=-Totaalvermogen","","Verwarmingscapaciteit-=-Totaalvermogen-=-Nom.-=-kW","kW","","","","","","13.5","15.5"]
["Behuizing","Behuizing-=-Kleur","","","","Niet gelakt (gegalvaniseerd)","Niet gelakt (gegalvaniseerd)","Niet gelakt (gegalvaniseerd)","Niet gelakt (gegalvaniseerd)","Niet gelakt (gegalvaniseerd)","Niet gelakt (gegalvaniseerd)","Niet gelakt (gegalvaniseerd)"]
["","Behuizing-=-Materiaal","","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["Afmetingen","Afmetingen-=-Unit","","Afmetingen-=-Unit-=-Hoogte-=-mm","mm","245","245","245","245","245","245","245"]
["","","","Afmetingen-=-Unit-=-Breedte-=-mm","mm","700","700","1000","1000","1400","1400","1400"]
["","","","Afmetingen-=-Unit-=-Diepte-=-mm","mm","800","800","800","800","800","800","800"]
["Gewicht","Gewicht-=-Unit-=-kg","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ventilator","Ventilator-=-Luchtdebiet","Ventilator-=-Luchtdebiet-=-Koelen","Ventilator-=-Luchtdebiet-=-Koelen-=-Hoog-=-m³/min","m³/min","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","","Ventilator-=-Luchtdebiet-=-Koeling","Ventilator-=-Luchtdebiet-=-Koeling-=-Middelhoog-=-m³/min","m³/min","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","","Ventilator-=-Luchtdebiet-=-Koelen-=-Laag-=-m³/min","m³/min","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","","Ventilator-=-Luchtdebiet-=-Verwarmen","Ventilator-=-Luchtdebiet-=-Verwarmen-=-Hoog-=-m³/min","m³/min","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","","Ventilator-=-Luchtdebiet-=-Verwarming","Ventilator-=-Luchtdebiet-=-Verwarming-=-Middelhoog-=-m³/min","m³/min","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","Ventilator-=-Luchtdebiet-=-Verwarmen","Ventilator-=-Luchtdebiet-=-Verwarmen-=-Laag-=-m³/min","m³/min","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","Ventilator-=-Externe statische druk","","Ventilator-=-Externe statische druk-=-Nom.-=-Pa","Pa","30","30","30","30","40","50","50"]
["Geluidsvermogenniveau","Geluidsvermogenniveau-=-Koelen-=-dBA","","","dBA","60.0","60.0","56.0","56.0","58.0","62.0","62.0"]
["Geluidsdrukniveau","Geluidsdrukniveau-=-Koelen","","Geluidsdrukniveau-=-Koelen-=-Hoog-=-dBA","dBA","35.0","35.0","30.0","30.0","34.0","37.0","37.0"]
["","Geluidsdrukniveau-=-Koeling","","Geluidsdrukniveau-=-Koeling-=-Middelhoog-=-dBA","dBA","32.0","32.0","28.0","28.0","32.0","35.0","35.0"]
["","","","Geluidsdrukniveau-=-Koelen-=-Laag-=-dBA","dBA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["","Geluidsdrukniveau-=-Verwarmen","","Geluidsdrukniveau-=-Verwarmen-=-Hoog-=-dBA","dBA","37.0","37.0","31.0","31.0","36.0","38.0","38.0"]
["","Geluidsdrukniveau-=-Verwarming","","Geluidsdrukniveau-=-Verwarming-=-Middelhoog-=-dBA","dBA","34.0","34.0","28.0","28.0","33.0","35.0","35.0"]
["","Geluidsdrukniveau-=-Verwarmen","","Geluidsdrukniveau-=-Verwarmen-=-Laag-=-dBA","dBA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["Leidingaansluitingen","Leidingaansluitingen-=-Vloeistof","","Leidingaansluitingen-=-Vloeistof-=-Buitendiameter-=-mm","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Leidingaansluitingen-=-Gas","","Leidingaansluitingen-=-Gas-=-Buitendiameter-=-mm","mm","9.52","12.70","12.70","15.90","15.90","15.90","15.90"]
["","Leidingaansluitingen-=-Drainage","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Afvoerhoogte-=-mm","mm","","","","625","625","625","625","625","625","625"]
["Regelsystemen","Regelsystemen-=-IR-afstandsbediening","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Regelsystemen-=-Bedrade afstandsbediening","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","4","4","4","4","4","4","4"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Screws","","","","40","40","40","40","40","40","40"]
["","Sealing pads","","","","5","5","5","5","5","5","5"]
["Voeding","Voeding-=-Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Spanningsvoeding-=-Frequentie-=-Hz","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Spanningsvoeding-=-Spanning-=-V","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]