{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":23,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ35D2VEB / FBQ35D2VEB / RZQG71L9V1B","FBQ100D2VEB / RZQG71L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG71L9V1B","FBQ100D2VEB / RZQG100L9V1B","FBQ140D2VEB / RZQG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQG100L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG100L9V1B","FBQ140D2VEB / RZQG125L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQG125L9V1B","FBQ71D2VEB / FBQ71D2VEB / RZQG125L9V1B","FBQ140D2VEB / RZQG140L9V1B","FBQ71D2VEB / RZQG71L9V1B (Archived)","FBQ60D2VEB / FBQ60D2VEB / RZQG125L9V1B (Archived)","FBQ125D2VEB / RZQG125L9V1B (Archived)"]
["Koelcapaciteit","Nom.","","kW","","","","","9.5 (2)","","","","","","","","","","","13.4 (2)"]
["Koeling","SEER","","","5.10","5.10","6.16","5.10","5.87","5.87","5.10","5.10","5.10","5.10","5.10","6.11","5.10","5.10","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","466","466","386","466","566","566","652","652","652","652","652","687","824","824","824"]
["","Vermogen","Pdesign","kW","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energieklasse","","","A","A","A++","A","A+","A+","A","A","A","A","A","A++","A","A","A"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.00","6.00","6.00","6.00","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.70","12.71","12.71","12.71"]
["","SCOP/A","","","3.80","3.80","4.31","3.80","4.78","4.78","3.80","3.80","3.80","3.80","3.80","4.28","3.80","3.80","3.80"]
["","Energieklasse","","","A","A","A+","A","A++","A++","A","A","A","A","A","A+","A","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,210","2,210","1,949","2,210","3,310","3,310","4,163","4,163","4,163","4,163","4,163","4,154","4,683","4,683","4,683"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","","","","","1,247"]
["","EER","","","","","","","3.81 (1)","","","","","","","","","","","3.35 (1)"]
["","COP","","","","","","","4.41 (1)","","","","","","","","","","","3.60 (1)"]
["","Richtlijn Energielabels","Koeling","","","","","","A"]
["","","Verwarming","","","","","","A"]
["Verwarmingscapaciteit","Nom.","","kW","","","","","10.80 (2)","","","","","","","","","","","15.50 (2)"]
["Opmerkingen","","","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","","","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","","","","","","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["Buitenunit","","","","","","","","","","","","","","","","","","","","RZQG71L9V1","RZQG125L9V1","RZQG125L9V1"]
["Koelcapaciteit","Nom.","","kW","","","","","","","","","","","","","","","","","6.8","","12.0"]
["Verwarmingscapaciteit","Nom.","","kW","","","","","","","","","","","","","","","","","7.5","","13.5"]
["Nominaal rendement","EER","","","","","","","","","","","","","","","","","","","3.53","","3.83"]
["","COP","","","","","","","","","","","","","","","","","","","3.96","","3.83"]
["","Jaarlijks energieverbruik","","kWh","","","","","","","","","","","","","","","","","963","","1567"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","","","","","","","","","","","","","","","","","A","","A"]
["","","Verwarming","","","","","","","","","","","","","","","","","","A","","A"]
["Koeling","Energieklasse","","","","","","","","","","","","","","","","","","","A++","A","A+"]
["","Vermogen","Pdesign","kW","","","","","","","","","","","","","","","","","6.80","12.00","12.00"]
["","SEER","","","","","","","","","","","","","","","","","","","6.16","5.10","5.83"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","","","","","","","","","","386","824","720"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","","","","","","","","","","","","","","","","A+","A","A+"]
["","Vermogen","Pdesign","kW","","","","","","","","","","","","","","","","","6.00","12.71","12.70"]
["","SCOP/A","","","","","","","","","","","","","","","","","","","4.35","3.80","4.37"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","","","","","","","","","","1931","4683","4069"]