{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ35D2VEB / FBQ35D2VEB / RZQSG71L3V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG100L9V1B","FBQ100D2VEB / RZQSG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L9V1B","FBQ125D2VEB / RZQSG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQSG125L9V1B","FBQ60D2VEB / FBQ60D2VEB / RZQSG125L9V1B","FBQ140D2VEB / RZQSG140L9V1B","FBQ71D2VEB / RZQSG71L3V1B (Archived)"]
["Koeling","SEER","","","5.10","5.10","5.61","5.10","5.47","4.80","4.80"]
["","Jaarlijks energieverbruik","","kWu/a","467","652","593","652","768","875","875"]
["","Vermogen","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Energieklasse","","","A","A","A+","A","A","B","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","4.15","3.80","4.01","3.80","3.80"]
["","Energieklasse","","","A","A","A+","A","A+","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,211","2,800","2,564","2,800","2,653","2,800","2,800"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["Koelcapaciteit","Nom.","","kW","","","9.5 (2)","","12.0 (2)","","","13.4 (2)"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","","","1,418","","1,858"]
["","EER","","","","","3.35 (1)","","3.23 (1)","","","3.06 (1)"]
["","COP","","","","","3.67 (1)","","3.63 (1)","","","3.40 (1)"]
["","Richtlijn Energielabels","Koeling","","","","A","","A"]
["","","Verwarming","","","","A","","A"]
["Verwarmingscapaciteit","Nom.","","kW","","","10.80 (2)","","13.50 (2)","","","15.50 (2)"]
["Opmerkingen","","","","","","(3) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","","(3) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels"]
["","","","","","","(4) - SEER en SCOP zijn conform EN 14825","","(4) - SEER en SCOP zijn conform EN 14825"]
["Buitenunit","","","","","","","","","","","","RZQSG71L3V1"]
["Koelcapaciteit","Nom.","","kW","","","","","","","","","6.8"]
["Verwarmingscapaciteit","Nom.","","kW","","","","","","","","","7.5"]
["Nominaal rendement","EER","","","","","","","","","","","3.30"]
["","COP","","","","","","","","","","","3.81"]
["","Jaarlijks energieverbruik","","kWh","","","","","","","","","1030"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","","","","","","","","","A"]
["","","Verwarming","","","","","","","","","","A"]
["Koeling","Energieklasse","","","","","","","","","","","A+"]
["","Vermogen","Pdesign","kW","","","","","","","","","6.80"]
["","SEER","","","","","","","","","","","5.84"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","","408"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","","","","","","","","A+"]
["","Vermogen","Pdesign","kW","","","","","","","","","6.00"]
["","SCOP/A","","","","","","","","","","","4.10"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","","2049"]