{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZAS-MY1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / AZAS100M7Y1B","FCAG125AVEB / AZAS125M7Y1B","FCAG140AVEB / AZAS140M7Y1B"]
["Koelcapaciteit","Nom.","","kW","","12.1 (1)","13.4 (1)"]
["Verwarmingscapaciteit","Nom.","","kW","","13.5 (2)","15.5 (2)"]
["Koeling","Vermogen","Pdesign","kW","","12.1","13.0"]
["","SEER","","","","5.40","6.00"]
["","Jaarlijks energieverbruik","","kWu/a","","1,345","1,300"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","","6.00","7.80"]
["","SCOP/A","","","","3.80","4.31"]
["","Jaarlijks energieverbruik","","kWu/a","","2,211","2,534"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Buitenunit","","","","AZAS100M7Y1B"]
["Koelcapaciteit","Nom.","","kW","9.50 (1)"]
["Verwarmingscapaciteit","Nom.","","kW","10.8 (2)"]
["Koeling","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","9.50"]
["","SEER","","","5.67"]
["","Jaarlijks energieverbruik","","kWu/a","586"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A"]
["","Vermogen","Pdesign","kW","6.00"]
["","SCOP/A","","","3.85"]
["","Jaarlijks energieverbruik","","kWu/a","2182"]
["Bereik van het energierendement","","","","A+++ ~ D"]