{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-A8"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXM50A5V1B8"]
["Koelcapaciteit","Nom.","","kW","5"]
["Verwarmingscapaciteit","Nom.","","kW","6"]
["Nominaal rendement","EER","","","3.45"]
["","COP","","","3.57"]
["","Jaarlijks energieverbruik","","kWu","725"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","B"]
["Koeling","Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","5"]
["","SEER","","","6.46"]
["","Jaarlijks energieverbruik","","kWu/a","271"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","4.36"]
["","SCOP/A","","","4.26"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.39"]
["","Jaarlijks energieverbruik","","kWu/a","1,433"]
["Opmerkingen","","","","(1) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","(2) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]