{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Koelcapaciteit","Nom.","","kW","5.00","5.70"]
["Verwarmingscapaciteit","Nom.","","kW","6.00","7.00"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","B"]
["Leidingaansluitingen","Drainage","UD","mm","VP25 (buitendiam. 32, binnendiam. 25)","VP25 (buitendiam. 32, binnendiam. 25)"]
["","Gas","Buitendiameter","mm","12.70","12.70"]
["","Vloeistof","Buitendiameter","mm","6.35","6.35"]
["Opmerkingen","","","","(1) - Bij normaal bedrijf: +22 °C / +32 °C","(1) - Bij normaal bedrijf: +22 °C / +32 °C"]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]