{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Koelcapaciteit","Nom.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Verwarmingscapaciteit","Nom.","","kW","","","","","","","","","","","","","","","","","7.50","","15.50"]
["Nominaal energierendement","EER","","","","","","","","","","","","","","","","3.30","3.30","3.30","3.39","3.39","2.50"]
["","COP","","","","","","","","","","","","","","","","","","","3.97","","3.61"]
["","Jaarlijks energieverbruik","","kWu","","","","","","","","","","","","","","","","","1,003"]
["","Richtlijn Energielabels","Koeling","","","","","","","","","","","","","","","","","","A"]
["","","Verwarming","","","","","","","","","","","","","","","","","","A"]
["Koeling","Energieklasse","","","","","","","","","","","","","","","","A","A","A","A++","A++"]
["","Vermogen","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10","5.10","6.72","6.80","6.44"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","","","","","","","467","467","467","355","350","1,249"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","","","","","","","","","","","","","A","A","A","A+","A+"]
["","Vermogen","Pdesign","kW","","","","","","","","","","","","","","6.00","6.00","6.00","6.33","6.33","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80","3.80","4.20","4.20","4.27"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","","","","","","","","","2,211","2,211","2,211","2,110","2,110","3,795"]
["Opmerkingen","","","","","","","","","","","","","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","","","","","","","","","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","","","","","","","","","","","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","","","","","","","","","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening","","(4) - Voor elektrische gegevens zie afzonderlijke tekening","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Bereik van het energierendement","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]