{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","FCAHG140FVEB","FCAHG100FVEB","FCAHG125FVEB","FCAHG71FVEB"]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","45","44","45"]
["","","Middelhoog","dBA","41","39","40"]
["","","Laag","dBA","37","33","35"]
["","Koelen","Middelhoog","dBA","41","39","40"]
["","","Laag","dBA","37","33","35"]
["","","Hoog","dBA","45","44","45"]
["Standaard-accessoires","Montage- en bedieningshandleiding","","","Montage- en bedieningshandleiding","Montage- en bedieningshandleiding","Montage- en bedieningshandleiding","Montage- en bedieningshandleiding"]
["","Montagehandleiding","","","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding"]
["Koelmiddel","GWP","","","675","675","675","675"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","9.52","9.52","9.52","9.52"]
["","Gas","Buitendiameter","mm","15.9","15.9","15.9"]
["","Afvoer","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Sierpaneel 4","Afmetingen","Diepte","mm","950","950","950","950"]
["","","Breedte","mm","950","950","950","950"]
["","","Hoogte","mm","50","50","50","50"]
["","Model","","","BYCQ140D7W1: wit met grijze lamellen","BYCQ140D7W1: wit met grijze lamellen","BYCQ140D7W1: wit met grijze lamellen","BYCQ140D7W1: wit met grijze lamellen"]
["","Kleur","","","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)"]
["","Gewicht","","kg","5.4","5.4","5.4","5.4"]
["Sound power level","Koelen","","dBA","61","61","61"]
["","Verwarmen","","dBA","61","61","61"]
["Afmetingen","Unit","Breedte","mm","840","840","840","840"]
["","","Diepte","mm","840","840","840","840"]
["","","Hoogte","mm","288","288","288","288"]
["Behuizing","Materiaal","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["Gewicht","Unit","","kg","26.0","26.0","26.0","25.0"]
["Sierpaneel","Gewicht","","kg","10","10","10"]
["","Model","","","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas"]
["","Afmetingen","Hoogte","mm","130","130","130"]
["","","Diepte","mm","950","950","950"]
["","","Breedte","mm","950","950","950"]
["","Kleur","","","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequentie","","Hz","50/60","50/60","50/60","50/60"]
["","Naam","","","VE","VE","VE","VE"]
["","Spanning","","V","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","(1) - De BYCQ140D7W1W heeft witte isolatie. Op witte isolatie is vuil sneller zichtbaar. Daarom is het niet aangeraden om decoratiepaneel BYCQ140D7W1W te installeren op plaatsen waar er veel vuil aanwezig is.","(1) - De BYCQ140D7W1W heeft witte isolatie. Op witte isolatie is vuil sneller zichtbaar. Daarom is het niet aangeraden om decoratiepaneel BYCQ140D7W1W te installeren op plaatsen waar er veel vuil aanwezig is.","(1) - De BYCQ140D7W1W heeft witte isolatie. Op witte isolatie is vuil sneller zichtbaar. Daarom is het niet aangeraden om decoratiepaneel BYCQ140D7W1W te installeren op plaatsen waar er veel vuil aanwezig is.","(1) - De BYCQ140D7W1W heeft witte isolatie. Op witte isolatie is vuil sneller zichtbaar. Daarom is het niet aangeraden om decoratiepaneel BYCQ140D7W1W te installeren op plaatsen waar er veel vuil aanwezig is."]
["","","","","(2) - Bevat gefluoreerde broeikasgassen","(2) - Bevat gefluoreerde broeikasgassen","(2) - Bevat gefluoreerde broeikasgassen","(2) - Bevat gefluoreerde broeikasgassen"]
["","","","","(3) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(3) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(3) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(3) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft."]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","","","","36"]
["","","Middelhoog","dBA","","","","33"]
["","","Laag","dBA","","","","29"]
["","Koelen","Middelhoog","dBA","","","","33"]
["","","Laag","dBA","","","","29"]
["","","Hoog","dBA","","","","36"]
["Leidingaansluitingen","Gas","Buitendiameter","mm","","","","15.9"]
["","Afvoer","","","","","","VP25 (I.D. 25/O.D. 32)"]
["Sound power level","Koelen","","dBA","","","","53"]
["","Verwarmen","","dBA","","","","53"]
["Sierpaneel","Gewicht","","kg","","","","10"]
["","Model","","","","","","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas"]
["","Afmetingen","Hoogte","mm","","","","130"]
["","","Diepte","mm","","","","950"]
["","","Breedte","mm","","","","950"]
["","Kleur","","","","","","Zuiver wit (RAL 9010)"]