{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG100GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Koelcapaciteit","Nom.","","kW","","6.80 (1)","9.50 (1)","","","12.0 (1)","","","13.4 (1)"]
["Koeling","SEER","","","6.91","6.91","7.00","7.00","5.10","6.61","6.61","5.10","6.75"]
["","ηs,c","","%","","","","","","","","","266.9"]
["","Jaarlijks energieverbruik","","kWu/a","345","345","475","475","652","636","636","824","1,191"]
["","Vermogen","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","12.0","12.0","12.0","13.4"]
["","Energieklasse","","","A++","A++","A++","A++","A","A++","A++","A"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.60","7.60","11.3","11.30","11.30","12.7","12.66","12.71","11.8"]
["","SCOP/A","","","4.54","4.54","4.80","4.80","3.80","4.63","4.63","3.80","4.38"]
["","Energieklasse","","","A+","A+","A++","A++","A","A++","A++","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,344","2,344","3,296","3,296","4,164","3,829","3,829","4,683","3,766"]
["","ηs,h","","%","","","","","","","","","172.1"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","","830","1,075","","","1,500"]
["","EER","","","","4.09 (3)","4.42 (3)","","","4.00 (3)","","","3.18 (3)"]
["","COP","","","","4.80 (3)","4.99 (3)","","","4.40 (3)","","","4.12 (3)"]
["","Richtlijn Energielabels","Koeling","","","A","A","","","A"]
["","","Verwarming","","","A","A","","","A"]
["Verwarmingscapaciteit","Nom.","","kW","","7.50 (2)","10.8 (2)","","","13.5 (2)","","","15.5 (2)"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m"]
["","","","","","(3) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(3) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(3) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(3) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]