{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Bereik van het energierendement","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Koelcapaciteit","Nom.","","kW","","","","","","6.80","13.40"]
["Koeling","SEER","","","","","","","","6.91","6.75"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","345","1,191"]
["","Vermogen","Pdesign","kW","","","","","","6.80","13.40"]
["","Energieklasse","","","","","","","","A++"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","","","","","","7.60","11.78"]
["","SCOP/A","","","","","","","","4.54","4.38"]
["","Energieklasse","","","","","","","","A+"]
["","Jaarlijks energieverbruik","","kWu/a","","","","","","2,344","3,766"]
["Nominaal energierendement","EER","","","","","","","","4.09","3.18"]
["Opmerkingen","","","","","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Koeling","ηs,c","","%","","","","","","","266.88"]
["Verwarming (gematigd klimaat)","ηs,h","","%","","","","","","","172.10"]
["Nominaal energierendement","COP","","","","","","","","","4.12"]
["Verwarmingscapaciteit","Nom.","","kW","","","","","","","15.50"]
["Opmerkingen","","","","","","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]