{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQSG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L8Y1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L8Y1B","FCQG125FVEB / RZQSG125L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L8Y1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L8Y1B","FCQG140FVEB / RZQSG140L7Y1B"]
["Koelcapaciteit","Nom.","","kW","9.5","","","12.0","","","","13.4"]
["Koeling","SEER","","","6.5","5.1","5.1","5.3","4.8","4.8","4.8"]
["","Jaarlijks energieverbruik","","kWu/a","512","652","652","793","875","875","875"]
["","Vermogen","Pdesign","kW","9.5","9.5","9.5","12","12","12","12"]
["","Energieklasse","","","A++","B","B","A","B","B","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.6","7.6","7.6","8.03","7.6","7.6","7.6"]
["","SCOP/A","","","4.1","3.8","3.8","4.01","3.8","3.8","3.8"]
["","Energieklasse","","","A+","A","A","A+","A","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,596","2,800","2,800","2,804","2,800","2,800","2,800"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","1,440","","","1,870","","","","2,225"]
["","EER","","","3.30","","","3.21","","","","3.01"]
["","COP","","","3.54","","","3.41","","","","3.41"]
["","Richtlijn Energielabels","Koeling","","A","","","A"]
["","","Verwarming","","A","","","B"]
["Verwarmingscapaciteit","Nom.","","kW","10.8","","","13.5","","","","15.5"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","(3) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","","","(3) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels"]
["","","","","(4) - SEER en SCOP zijn conform EN 14825","","","(4) - SEER en SCOP zijn conform EN 14825"]
["","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]