{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":116,"n_cols":9,"rows_kept":116,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["","","","Laag","dBA","","33","35","37"]
["","Koelen","","Laag","dBA","","33","35","37"]
["","","","Hoog","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["Standaard-accessoires","Bedieningshandleiding","","","","","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding"]
["","Montagehandleiding","","","","","Montagehandleiding","Montagehandleiding","Montagehandleiding"]
["","Afvoerslang","","","","","Afvoerslang","Afvoerslang","Afvoerslang"]
["","Klem voor afvoerslang","","","","","Klem voor afvoerslang","Klem voor afvoerslang","Klem voor afvoerslang"]
["","Sluitring voor ophangbeugel","","","","","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel"]
["","Schroeven","","","","","Schroeven","Schroeven","Schroeven"]
["","Isolatie voor fitting","","","","","2","2","2"]
["","Afdichtingskussens","","","","","4","4","4"]
["","Afdichtingskussen voor de afvoer","","","","","Afdichtingskussen voor de afvoer","Afdichtingskussen voor de afvoer","Afdichtingskussen voor de afvoer"]
["","Klemmen","","","","","Klemmen","Klemmen","Klemmen"]
["Besturingssystemen","Bedrade afstandsbediening","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","","15.9","15.9","15.9"]
["","Afvoer","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Sierpaneel 4","Afmetingen","","Diepte","mm","","50","50","50"]
["","","","Breedte","mm","","950","950","950"]
["","","","Hoogte","mm","","950","950","950"]
["","Model","","","","","BYCQ140D7W1: wit met grijze lamellen","BYCQ140D7W1: wit met grijze lamellen","BYCQ140D7W1: wit met grijze lamellen"]
["","Kleur","","","","","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)"]
["","Gewicht","","","kg","","5.4","5.4","5.4"]
["Sound power level","Koelen","","","dBA","","61","61","61"]
["","Verwarmen","","","dBA","","61","61","61"]
["Afmetingen","Unit","","Breedte","mm","","840","840","840"]
["","","","Diepte","mm","","840","840","840"]
["","","","Hoogte","mm","","288","288","288"]
["Behuizing","Materiaal","","","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["Gewicht","Unit","","","kg","","26","26","26"]
["Sierpaneel","Gewicht","","","kg","","10.3","10.3","10.3"]
["","Model","","","","","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas"]
["","Afmetingen","","Hoogte","mm","","130","130","130"]
["","","","Diepte","mm","","950","950","950"]
["","","","Breedte","mm","","950","950","950"]
["","Kleur","","","","","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)","Zuiver wit (RAL 9010)"]
["Power supply","Fase","","","","","1~","1~","1~"]
["","Frequentie","","","Hz","","50","50","50"]
["","Naam","","","","","VE","VE","VE"]
["","Spanning","","","V","","220-240","220-240","220-240"]
["Opmerkingen","","","","","","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft."]
["","","","","","","(2) - De BYCQ140D7W1W heeft witte isolatie. Op witte isolatie is vuil sneller zichtbaar. Daarom is het niet aangeraden om decoratiepaneel BYCQ140D7W1W te installeren op plaatsen waar er veel vuil aanwezig is.","(2) - De BYCQ140D7W1W heeft witte isolatie. Op witte isolatie is vuil sneller zichtbaar. Daarom is het niet aangeraden om decoratiepaneel BYCQ140D7W1W te installeren op plaatsen waar er veel vuil aanwezig is.","(2) - De BYCQ140D7W1W heeft witte isolatie. Op witte isolatie is vuil sneller zichtbaar. Daarom is het niet aangeraden om decoratiepaneel BYCQ140D7W1W te installeren op plaatsen waar er veel vuil aanwezig is."]
["","","","","","","(3) - BYCQ140D7W1: standaardpaneel in zuiver wit met grijze lamellen; BYCQ140D7W1W: standaardpaneel in zuiver wit met witte lamellen; BYCQ140D7GW1: zelfreinigend paneel in zuiver wit.","(3) - BYCQ140D7W1: standaardpaneel in zuiver wit met grijze lamellen; BYCQ140D7W1W: standaardpaneel in zuiver wit met witte lamellen; BYCQ140D7GW1: zelfreinigend paneel in zuiver wit.","(3) - BYCQ140D7W1: standaardpaneel in zuiver wit met grijze lamellen; BYCQ140D7W1W: standaardpaneel in zuiver wit met witte lamellen; BYCQ140D7GW1: zelfreinigend paneel in zuiver wit."]
["Behuizing","Materiaal","","","","Gegalvaniseerde staalplaat"]
["Afmetingen","Unit","","Hoogte","mm","288"]
["","","","Breedte","mm","840"]
["","","","Diepte","mm","840"]
["Gewicht","Unit","","","kg","25"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Laag","m³/min","12.2"]
["","","Verwarmen","Hoog","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Laag","m³/min","12.2"]
["Geluidsvermogenniveau","Koelen","","","dBA","53"]
["","Verwarmen","","","dBA","53"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Laag","dBA","29"]
["","Verwarmen","","Hoog","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Laag","dBA","29"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52"]
["","Gas","","Buitendiameter","mm","15.9"]
["","Drainage","","","","VP25 (I.D. 25/O.D. 32)"]
["Sierpaneel","Model","","","","BYCQ140D7GFW1: zelfreinigend paneel met filter met fijne maas"]
["","Kleur","","","","Zuiver wit (RAL 9010)"]
["","Afmetingen","","Hoogte","mm","130"]
["","","","Breedte","mm","950"]
["","","","Diepte","mm","950"]
["","Gewicht","","","kg","10.3"]
["Sierpaneel 2","Model","","","","BYCQ140DG: zelfreinigend paneel"]
["","Kleur","","","","Zuiver wit (RAL 9010)"]
["","Afmetingen","","Hoogte","mm","130"]
["","","","Breedte","mm","950"]
["","","","Diepte","mm","950"]
["","Gewicht","","","kg","10.3"]
["Sierpaneel 3","Model","","","","BYCQ140DW: volledig wit"]
["","Kleur","","","","Zuiver wit (RAL 9010)"]
["","Afmetingen","","Hoogte","mm","50"]
["","","","Breedte","mm","950"]
["","","","Diepte","mm","950"]
["","Gewicht","","","kg","5.4"]
["Sierpaneel 4","Model","","","","BYCQ140D: wit met grijze lamellen"]
["","Kleur","","","","Zuiver wit (RAL 9010)"]
["","Afmetingen","","Hoogte","mm","950"]
["","","","Breedte","mm","950"]
["","","","Diepte","mm","50"]
["","Gewicht","","","kg","5.4"]
["Besturingssystemen","Infrared remote control","","","","BRC7FA532F"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC1D52, BRC1E52A/B"]
["Standaard-accessoires","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Voeding","Naam","","","","VE"]
["","Fase","","","","1~"]
["Spanningsvoeding","Spanningsvoeding-=-Frequentie","","Frequentie","","50"]
["","Spanningsvoeding-=-Spanning","","Spanning","","220-240"]