{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Koelcapaciteit","Nom.","","kW","12.5 (3)"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","9.52"]
["","Gas","Buitendiameter","mm","15.9"]
["","Afvoer","UD","mm","26"]
["Koeling","SEER","","","3.50"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Richtlijn Energielabels","Koeling","","B"]
["","","Verwarming","","A"]
["Verwarmingscapaciteit","Nom.","","kW","14.0 (4)"]
["Opmerkingen","","","","(1) - Energielabel: schaalverdeling van A (meest efficiënt) tot G (minst efficiënt)"]
["","","","","(2) - Jaarlijks energieverbruik: op basis van een gemiddelde van 500 bedrijfsuren per jaar bij vollast (nominale omstandigheden)"]
["","","","","(3) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(5) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]