{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B"]
[]
[]
[]
[]
["","","","","","FDQ125B8V3B9","FDQ200B8V3B9","FDQ250B8V3B9"]
["Koelcapaciteit","Totaalvermogen","","Nom.","kW","","20.0","24.1"]
["Verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","","23.0","26.4"]
["Behuizing","Colour","","","","Ongelakt","Ongelakt","Ongelakt"]
["","Materiaal","","","","Gegalvaniseerd staal","Gegalvaniseerd staal","Gegalvaniseerd staal"]
["Afmetingen","Unit","","Hoogte","mm","350","450","450"]
["","","","Breedte","mm","1,400","1,400","1,400"]
["","","","Diepte","mm","662","900","900"]
["Gewicht","Unit","","","kg","59.0","89.0","94.0"]
["Vereiste plafondruimte >","mm","","","","350","450","450"]
["Ventilator","Luchtdebiet","Koelen","Nom.","m³/min","43.0"]
["","","","Middelhoog","m³/min","","69.0","89.0"]
["","","Verwarmen","Nom.","m³/min","43.0"]
["","","","Middelhoog","m³/min","","69.0","89.0"]
["","Externe statische druk","","Hoog","Pa","150","250","250"]
["","","","Nom.","Pa","150","250","250"]
["","","","Laag","Pa","150","250","250"]
["Geluidsvermogenniveau","Koelen","","","dBA","75.0","81.0","82.0"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","44.0","45.0","47.0"]
["","Verwarmen","","Laag","dBA","44.0","45.0","47.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","12.70"]
["","Gas","","Buitendiameter","mm","15.9","22.2","22.2"]
["","Drainage","","","","","OD Ø25.0","OD Ø25.0"]
["Control systems","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standaard-accessoires","Montage- en bedieningshandleiding","","","","1","1","1"]
["Power supply","Naam","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","230","230 +/-10%","230 +/-10%"]
["Opmerkingen","","","","","(1) - De geluidswaarden worden gemeten in een semi-echoloze ruimte met correcties.","(1) - De geluidswaarden worden gemeten in een semi-echoloze ruimte met correcties.","(1) - De geluidswaarden worden gemeten in een semi-echoloze ruimte met correcties."]
["","","","","","(2) - Het geluidsdrukniveau wordt gemeten met een microfoon op 1 m afstand van de unit.","(2) - Het geluidsdrukniveau wordt gemeten met een microfoon op 1 m afstand van de unit.","(2) - Het geluidsdrukniveau wordt gemeten met een microfoon op 1 m afstand van de unit."]
["","","","","","(3) - Het geluidsdrukniveau is een relatieve waarde, die afhankelijk is van de afstand en de akoestische omgeving. Zie de geluidsniveautekeningen voor meer bijzonderheden.","(3) - Het geluidsdrukniveau is een relatieve waarde, die afhankelijk is van de afstand en de akoestische omgeving. Zie de geluidsniveautekeningen voor meer bijzonderheden.","(3) - Het geluidsdrukniveau is een relatieve waarde, die afhankelijk is van de afstand en de akoestische omgeving. Zie de geluidsniveautekeningen voor meer bijzonderheden."]
["","","","","","(4) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(4) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(4) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft."]
["","","","","","(5) - Voor meer informatie raadpleegt u het aansluitschema, naamplaat en installatiehandleiding.","(5) - Voor meer informatie raadpleegt u het aansluitschema, naamplaat en installatiehandleiding.","(5) - Voor meer informatie raadpleegt u het aansluitschema, naamplaat en installatiehandleiding."]