{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Koelcapaciteit","Min.","","kW","","1.70"]
["","Nom.","","kW","","6.00"]
["","Max.","","kW","","6.50"]
["Verwarmingscapaciteit","Min.","","kW","","1.70"]
["","Nom.","","kW","","7.00"]
["","Max.","","kW","","7.10"]
["Nominaal energierendement","EER","","","","2.93"]
["","COP","","","","3.21"]
["","Jaarlijks energieverbruik","","kWh","","1,024"]
["","Richtlijn Energielabels","Koeling","","","C"]
["","","Verwarming","","","C"]
["Koeling","Energieklasse","","","","A"]
["","Vermogen","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","Jaarlijks energieverbruik","","kWu/a","","378"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","A"]
["","Vermogen","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Jaarlijks energieverbruik","","kWu/a","","1,693"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(3) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","(4) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Koelcapaciteit","Min.","","kW","1.70"]
["","Nom.","","kW","5.00"]
["","Max.","","kW","5.30"]
["Verwarmingscapaciteit","Min.","","kW","1.70"]
["","Nom.","","kW","5.80"]
["","Max.","","kW","6.00"]
["Nominaal rendement","EER","","","3.06"]
["","COP","","","3.10"]
["","Jaarlijks energieverbruik","","kWh","816"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","B"]
["","","Verwarming","","D"]
["Koeling","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["","Jaarlijks energieverbruik","","kWu/a","303"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A"]
["","Vermogen","Pdesign","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.55"]
["","Jaarlijks energieverbruik","","kWu/a","1424"]
["Bereik van het energierendement","","","","A+++ ~ D"]