{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","35","35","38","38"]
["","","Middelhoog","dBA","33","33","35","35"]
["","","Laag","dBA","27","27","30","30"]
["","Koelen","Middelhoog","dBA","33","33","35","35"]
["","","Laag","dBA","27","27","30","30"]
["","","Hoog","dBA","35","35","38","38"]
["Standaard-accessoires","Montagehandleiding","","","1","1","1","1"]
["","Bedieningshandleiding","","","1","1","1","1"]
["","Isolatie voor fitting","","","1","1","1","1"]
["","Afdichtingskussen","","","1","1","1","1"]
["","Klemmetaal","","","1","1","1","1"]
["","Afvoerslang","","","1","1","1","1"]
["","Sluitring voor ophangbeugel","","","8","8","8","8"]
["","Afdichtingsmateriaal","","","2","2","2","2"]
["","Klemmen","","","6","6","6","6"]
["","Sluitring bevestigingsplaat","","","4","4","4","4"]
["","Schroeven voor kanaalflenzen","","","1","1","1","1"]
["","Luchtfilter","","","1","1","1","1"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","Buitendiameter","mm","9.50","9.50","12.70","12.70"]
["","Afvoer","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Power input","Koelen","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Verwarmen","Nom.","kW","0.036","0.036","0.060","0.060"]
["Sound power level","Koelen","","dBA","53","53","55","56"]
["","Verwarmen","","dBA","53","53","55","56"]
["Afmetingen","Unit","Breedte","mm","750","750","1,150","1,150"]
["","","Diepte","mm","620","620","620","620"]
["","","Hoogte","mm","200","200","200","200"]
["Gewicht","Unit","","kg","21","21","28","28"]
["Ventilator","Externe statische druk","Nom.","Pa","30","30","40","40"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frequentie","","Hz","50","50","50","50"]
["","Spanning","","V","220-240","220-240","220-240","220-240"]