{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-C / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60CVMB / RXS60F3V1B"]
["Koelcapaciteit","Min.","","kW","1.7"]
["","Max.","","kW","6.5"]
["","Nom.","","kW","6.0 (1)"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","6.35"]
["","Gas","Buitendiameter","mm","12.7"]
["","Drain","OD","mm","26"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","1,065"]
["","EER","","","2.82"]
["","COP","","","3.02"]
["","Richtlijn Energielabels","Koeling","","C"]
["","","Verwarming","","D"]
["Verwarmingscapaciteit","Nom.","","kW","7.0 (2)"]
["","Min.","","kW","1.7"]
["","Max.","","kW","8.0"]
["Opmerkingen","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB, 24°CWB; equivalente leidinglengte: 7,5m"]
["","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m"]
["","","","","(3) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]