{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60F2VEB / RXS60F4V1B"]
["Koelcapaciteit","Min.","","kW","1.7"]
["","Max.","","kW","6.5"]
["","Nom.","","kW","6.0 (2)"]
["Piping connections","Vloeistof","Buitendiameter","mm","6.35"]
["","Gas","Buitendiameter","mm","12.7"]
["","Afvoer","OD","mm","VP20 (buitendiam. 26, binnendiam. 20)"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","1,030"]
["","EER","","","2.91 (1)"]
["","COP","","","3.21 (1)"]
["","Richtlijn Energielabels","Koeling","","C"]
["","","Verwarming","","C"]
["Verwarmingscapaciteit","Nom.","","kW","7.0 (3)"]
["","Min.","","kW","1.7"]
["","Max.","","kW","8.0"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m"]
["","","","","(3) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m"]
["","","","","(4) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]