{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","38"]
["","","Middelhoog","dBA","36"]
["","","Laag","dBA","30"]
["","Koelen","Middelhoog","dBA","36"]
["","","Laag","dBA","30"]
["","","Hoog","dBA","38"]
["Standaard-accessoires","Montagehandleiding","","","1"]
["","Bedieningshandleiding","","","1"]
["","Isolatie voor fitting","","","1"]
["","Afdichtingskussen","","","1"]
["","Klemmetaal","","","1"]
["","Afvoerslang","","","1"]
["","Sluitring voor ophangbeugel","","","8"]
["","Afdichtingsmateriaal","","","2"]
["","Klemmen","","","6"]
["","Sluitring bevestigingsplaat","","","4"]
["","Schroeven voor kanaalflenzen","","","1"]
["","Luchtfilter","","","1"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","6.35"]
["","Gas","Buitendiameter","mm","12.7"]
["","Afvoer","","","VP20 (I.D. 20/O.D. 26)"]
["Opgenomen vermogen","Koelen","Nom.","kW","0.060"]
["","Verwarmen","Nom.","kW","0.060"]
["Geluidsvermogenniveau","Koelen","","dBA","55"]
["","Verwarmen","","dBA","55"]
["Afmetingen","Unit","Breedte","mm","1,150"]
["","","Diepte","mm","620"]
["","","Hoogte","mm","200"]
["Gewicht","Unit","","kg","30.0"]
["Ventilator","Externe statische druk","Nom.","Pa","40"]
["Power supply","Fase","","","1~"]
["","Frequentie","","Hz","50/60"]
["","Naam","","","VE"]
["","Spanning","","V","220-240"]
["Opmerkingen","","","","(1) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden."]