{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Koelcapaciteit","Nom.","","kW","","5.70"]
["Verwarmingscapaciteit","Nom.","","kW","","7.00"]
["Nominaal energierendement","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Jaarlijks energieverbruik","","kWu","","934"]
["","Richtlijn Energielabels","Koeling","","","B"]
["","","Verwarming","","","B"]
["Koeling","Energieklasse","","","","A+"]
["","Vermogen","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Jaarlijks energieverbruik","","kWu/a","","347"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","A+"]
["","Vermogen","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Jaarlijks energieverbruik","","kWu/a","","1,372"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(3) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","(4) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Koelcapaciteit","Nom.","","kW","5.00"]
["Verwarmingscapaciteit","Nom.","","kW","5.80"]
["Nominaal rendement","EER","","","3.24"]
["","COP","","","3.49"]
["","Jaarlijks energieverbruik","","kWu","771"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","B"]
["Koeling","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["","Jaarlijks energieverbruik","","kWu/a","292"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A"]
["","Vermogen","Pdesign","kW","3.84"]
["","SCOP/A","","","3.90"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.51"]
["","Jaarlijks energieverbruik","","kWu/a","1377"]
["Bereik van het energierendement","","","","A+++ ~ D"]