{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Behuizing","Materiaal","","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["Afmetingen","Unit","","Hoogte","mm","260","260","260","260"]
["","","","Breedte","mm","575","575","575","575"]
["","","","Diepte","mm","575","575","575","575"]
["Gewicht","Unit","","","kg","16.0","16.0","17.5","17.5"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","9.0","10.0","12.0","14.5"]
["","","Koeling","Middelhoog","m³/min","8.0","8.5","10.0","12.5"]
["","","","Laag","m³/min","6.5","6.5","7.5","9.5"]
["","","Verwarmen","Hoog","m³/min","9.0","10.0","12.0","14.5"]
["","","Verwarming","Middelhoog","m³/min","8.0","8.5","10.0","12.5"]
["","","Verwarmen","Laag","m³/min","6.5","6.5","7.5","9.5"]
["Geluidsvermogenniveau","Koelen","","","dBA","48","51","56","60"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","31.0","34.0","39.0","43.0"]
["","Koeling","","Middelhoog","dBA","28.5","30.5","34.0","40.0"]
["","","","Laag","dBA","25.0","25.0","27.0","32.0"]
["","Verwarmen","","Hoog","dBA","31.0","34.0","39.0","43.0"]
["","Verwarming","","Middelhoog","dBA","28.5","30.5","34.0","40.0"]
["","Verwarmen","","Laag","dBA","25.0","25.0","27.0","32.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.52","9.52","12.70","12.70"]
["","Drainage","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sierpaneel","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Kleur","","","","Wit (N9.5)","Wit (N9.5)","Wit (N9.5)","Wit (N9.5)"]
["","Afmetingen","","Hoogte","mm","46","46","46","46"]
["","","","Breedte","mm","620","620","620","620"]
["","","","Diepte","mm","620","620","620","620"]
["","Gewicht","","","kg","2.8","2.8","2.8","2.8"]
["Sierpaneel 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Kleur","","","","Zilver","Zilver","Zilver","Zilver"]
["","Afmetingen","","Hoogte","mm","46","46","46","46"]
["","","","Breedte","mm","620","620","620","620"]
["","","","Diepte","mm","620","620","620","620"]
["","Gewicht","","","kg","2.8","2.8","2.8","2.8"]
["Sierpaneel 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Kleur","","","","Wit (RAL9010)","Wit (RAL9010)","Wit (RAL9010)","Wit (RAL9010)"]
["","Afmetingen","","Hoogte","mm","55","55","55","55"]
["","","","Breedte","mm","700","700","700","700"]
["","","","Diepte","mm","700","700","700","700"]
["","Gewicht","","","kg","2.7","2.7","2.7","2.7"]
["Sierpaneel 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Kleur","","","","WIT (RAL9010)","Wit (RAL9010)","Wit (RAL9010)","Wit (RAL9010)"]
["","Afmetingen","","Hoogte","mm","55","55","55","55"]
["","","","Breedte","mm","700","700","700","700"]
["","","","Diepte","mm","700","700","700","700"]
["","Gewicht","","","kg","2.7","2.7","2.7","2.7"]
["Regelsystemen","IR-afstandsbediening","","","","BRC7EB530 (standaard paneel), BRC7F530W (wit paneel), BRC7F530S (grijs paneel)","BRC7EB530 (standaard paneel), BRC7F530W (wit paneel), BRC7F530S (grijs paneel)","BRC7EB530 (standaard paneel), BRC7F530W (wit paneel), BRC7F530S (grijs paneel)","BRC7EB530 (standaard paneel), BRC7F530W (wit paneel), BRC7F530S (grijs paneel)"]
["","Bedrade afstandsbediening","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standaard-accessoires","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Voeding","Fase","","","","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]