{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-K"]
[]
[]
[]
[]
["","","","","FFQ25B9V1B / RXS25K2V1B","FFQ25B9V1B / RXS25K3V1B","FFQ35B9V1B / RXS35K2V1B","FFQ50B9V1B / RXS50K2V1B"]
["Koelcapaciteit","Nom.","","kW","2.50 (3)","2.50 (3)","3.4 (3)","4.7 (3)"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","","","6.35","6.35"]
["","Gas","Buitendiameter","mm","","","9.5","12.7"]
["","Afvoer","UD","mm","","","VP20 (buitendiam. 26, binnendiam. 20)","VP20 (buitendiam. 26, binnendiam. 20)"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","365","365","650","900"]
["","EER","","","3.43","3.43","2.62","2.61"]
["","COP","","","3.48","3.48","2.81","2.81"]
["","Richtlijn Energielabels","Koeling","","A","A","D","D"]
["","","Verwarming","","B","B","D","D"]
["Verwarmingscapaciteit","Nom.","","kW","3.20 (4)","3.20 (4)","4.5 (4)","5.5 (4)"]
["Opmerkingen","","","","(1) - Energielabel: schaalverdeling van A (meest efficiënt) tot G (minst efficiënt)","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Jaarlijks energieverbruik: op basis van een gemiddelde van 500 bedrijfsuren per jaar bij vollast (nominale omstandigheden)","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","(3) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(5) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]