{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RXM50A5V1B","FHA50AVEB99 / RXM50A5V1B","FHA60AVEB98 / RXM60A5V1B"]
["Koelcapaciteit","Nom.","","kW","5.00","5.00","5.7"]
["Verwarmingscapaciteit","Nom.","","kW","6.00","6.00","7.2"]
["Nominaal rendement","EER","","","3.21","3.21","3.29"]
["","COP","","","3.35","3.35","3.32"]
["","Jaarlijks energieverbruik","","kWu","779","779","866"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A","A"]
["","","Verwarming","","C","C","C"]
["Koeling","Energieklasse","","","A+","A+","A+"]
["","Vermogen","Pdesign","kW","5.00","5.00","5.7"]
["","SEER","","","5.92","5.92","6.08"]
["","Jaarlijks energieverbruik","","kWu/a","295","295","328"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A","A","A"]
["","Vermogen","Pdesign","kW","4.35","4.35","4.71"]
["","SCOP/A","","","3.86","3.86","3.87"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.85","3.85","4.08"]
["","Jaarlijks energieverbruik","","kWu/a","1577","1577","1704"]
["Opmerkingen","","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]