{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":26,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9)"]
[]
[]
[]
[]
["","","","","","FHA35AVEB99","FHA35AVEB98","FHA35AVEB9","FHA50AVEB9","FHA50AVEB99","FHA50AVEB98","FHA60AVEB9","FHA60AVEB99","FHA60AVEB98","FHA71AVEB99","FHA71AVEB9","FHA71AVEB98","FHA100AVEB9","FHA100AVEB","FHA100AVEB8","FHA125AVEB","FHA125AVEB8","FHA125AVEB9","FHA140AVEB","FHA140AVEB8"]
["Koelcapaciteit","Totale capaciteit","","Nom.","kW","","","","","","","","","","","","","","","","","14.00","","","15.40"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit","Wit","Wit","Wit","","Wit","","","Wit","Wit","Wit","Wit","","Wit","","","Wit"]
["","Materiaal","","","","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","","Kunsthars, metaalplaat","","","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","","Kunsthars, metaalplaat","","","Kunsthars, metaalplaat"]
["Afmetingen","Unit","","Hoogte","mm","235","235","235","235","235","235","235","","235","","","235","235","235","235","","235","","","235"]
["","","","Breedte","mm","960","960","960","960","960","960","1270","","1270","","","1270","1590","1590","1590","","1590","","","1590"]
["","","","Diepte","mm","690","690","690","690","690","690","690","","690","","","690","690","690","690","","690","","","690"]
["Gewicht","Unit","","","kg","24.0","26","24","25","25.0","27","31","31.0","32","32.0","32","34","38.0","38.0","41","38.0","41","38.0","38.0","41","38.0"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","14.0","14.0","14.0","15.0","15.0","15.0","19.5","","19.5","","","20.5","28.0","28.0","28.0","","31.0","","","34.0"]
["","","Koeling","Middelhoog","m³/min","11.5","11.5","11.5","12.0","12.0","12.0","15.0","","15.0","","","17.0","24.0","24.0","24.0","","27.0","","","29.0"]
["","","","Laag","m³/min","10.0","10.0","10.0","10.0","10.0","10.0","11.5","","11.5","","","14.0","20.0","20.0","20.0","","23.0","","","24.0"]
["","","Verwarmen","Hoog","m³/min","14.0","14.0","14.0","15.0","15.0","15.0","19.5","","19.5","","","20.5","28.0","28.0","28.0","","31.0","","","34.0"]
["","","Verwarming","Middelhoog","m³/min","11.5","11.5","11.5","12.0","12.0","12.0","15.0","","15.0","","","17.0","24.0","24.0","24.0","","27.0","","","29.0"]
["","","Verwarmen","Laag","m³/min","10.0","10.0","10.0","10.0","10.0","10.0","11.5","","11.5","","","14.0","20.0","20.0","20.0","","23.0","","","24.0"]
["Geluidsvermogenniveau","Koelen","","","dBA","53","53.0","53.0","54.0","54","54.0","54.0","","54.0","","","55.0","60","60","60.0","","62.0","","","64.0"]
["","Verwarmen","","","dBA","","53.0","","","","54.0","","","54.0","","","55.0","","","60.0","","62.0","","","64.0"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","36","36.0","36.0","37.0","37","37.0","37.0","","37.0","","","38.0","42","42","42.0","","44.0","","","46.0"]
["","Koeling","","Middelhoog","dBA","34","34.0","34.0","35.0","35","35.0","35.0","","35.0","","","36.0","38","38","38.0","","41.0","","","42.0"]
["","","","Laag","dBA","31","31.0","31.0","32.0","32","32.0","33.0","","33.0","","","34.0","34","34","34.0","","37.0","","","38.0"]
["","Verwarmen","","Hoog","dBA","36","36.0","36.0","37.0","37","37.0","37.0","","37.0","","","38.0","42","42","42.0","","44.0","","","46.0"]
["","Verwarming","","Middelhoog","dBA","31","31.0","31.0","32.0","32","32.0","33.0","","33.0","","","34.0","34","34","34.0","","37.0","","","38.0"]
["","Verwarmen","","Nom.","dBA","34","34.0","34.0","35.0","35","35.0","35.0","","35.0","","","36.0","38","38","38.0","","41.0","","","42.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.40","6.35","6.35","6.35","6.40","6.35","6.35","","6.35","","","9.52","9.52","9.52","9.52","","9.52","","","9.52"]
["","Gas","","Buitendiameter","mm","9.50","9.50","9.5","12.7","12.7","12.70","12.7","","12.70","","","15.90","15.9","15.9","15.90","","15.90","","","15.90"]
["","Drainage","","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20","","VP20","","","VP20","VP20","VP20","VP20","","VP20","","","VP20"]
["Regelsystemen","IR-afstandsbediening","","","","BRC7GA53, BRC7GA56","BRC7F530W (wit paneel), BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7F530W (wit paneel), BRC7GA56","BRC7GA53, BRC7GA56","","BRC7F530W (wit paneel), BRC7GA56","","","BRC7F530W (wit paneel), BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7F530W (wit paneel), BRC7GA56","","BRC7F530W (wit paneel), BRC7GA56","","","BRC7F530W (wit paneel), BRC7GA56"]
["","Bedrade afstandsbediening","","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~","1~","","1~","","","1~","1~","1~","1~","","1~","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50/60","50","50","50","50/60","50","","50/60","","","50/60","50","50","50/60","","50/60","","","50/60"]
["","Spanning","","","V","220-240","220-240/220","220-240","220-240","220-240","220-240/220","220-240","","220-240/220","","","220-240/220","220-240","220-240","220-240/220","","220-240/220","","","220-240/220"]
["Standaard-accessoires","Thermal insulation tube","","","","2","2","2","2","2","2","2","","2","","","2","","","","","2","","","2"]
["","Resin bushing","","","","1","1","1","1","1","1","1","","1","","","1","","","","","1","","","1"]
["","Wiring fixture","","","","2","2","2","2","2","2","2","","2","","","2","","","","","2","","","2"]
["","Hose band","","","","1","1","1","1","1","1","1","","1","","","1","1","1","1","","1","","","1"]
["","Wire clamp material","","","","7","7","7","7","7","7","7","","7","","","7","7","7","7","","7","","","7"]
["","Drain hose","","","","1","1","1","1","1","1","1","","1","","","1","","","","","1","","","1"]
["","Screws","","","","2","2","2","2","2","2","2","","2","","","2","","","","","2","","","2"]
["","Sealing pad (large)","","","","1","","1","1","1","","1"]
["","Sealing pad (small)","","","","1","","1","1","1","","1"]
["","Washer","","","","8","8","8","8","8","8","8","","8","","","8","","","","","8","","","8"]
["Opmerkingen","","","","","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening","","","","","","","","","","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Standaard-accessoires","General safety precautions","","","","","1","","","","1","","","1","","","1","","","1","","1","","","1"]
["","Installation and operation manual","","","","","1","","","","1","","","1","","","1","","","","","1","","","1"]
["","Paper pattern for installation","","","","","1","","","","1","","","1","","","1","","","","","1","","","1"]
["","Sealing material","","","","","6","","","","6","","","6","","","6","","","","","6","","","6"]
["","Thermische isolatiebuis","","","","","","","","","","","","","","","","2","2","2"]
["","Mof van kunsthars","","","","","","","","","","","","","","","","1","1","1"]
["","Bedradingsklem","","","","","","","","","","","","","","","","2","2","2"]
["","Afvoerslang","","","","","","","","","","","","","","","","1","1","1"]
["","Schroeven","","","","","","","","","","","","","","","","2","2","2"]
["","Afdichtingskussen (groot)","","","","","","","","","","","","","","","","1","1"]
["","Afdichtingskussen (klein)","","","","","","","","","","","","","","","","1","1"]
["","Sluitring","","","","","","","","","","","","","","","","8","8","8"]
["","Montage- en bedieningshandleiding","","","","","","","","","","","","","","","","","","1"]
["","Papieren montagemal","","","","","","","","","","","","","","","","","","1"]
["","Afdichtingsmateriaal","","","","","","","","","","","","","","","","","","6"]