{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Koelcapaciteit","Nom.","","kW","3.40"]
["Koeling","SEER","","","6.24"]
["","Jaarlijks energieverbruik","","kWu/a","191"]
["","Vermogen","Pdesign","kW","3.40"]
["","Energieklasse","","","A++"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Energieklasse","","","A+"]
["","Jaarlijks energieverbruik","","kWu/a","979"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","A"]
["Verwarmingscapaciteit","Nom.","","kW","4.00"]
["Opmerkingen","","","","(1) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","(2) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(3) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(4) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Outdoor unit","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Koelcapaciteit","Nom.","","kW","","5.00","5.70"]
["Verwarmingscapaciteit","Nom.","","kW","","6.00","7.20"]
["Nominaal rendement","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Jaarlijks energieverbruik","","kWu","","780","867"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","","B","A"]
["","","Verwarming","","","C","C"]
["Koeling","Energieklasse","","","","A+","A+"]
["","Vermogen","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Jaarlijks energieverbruik","","kWu/a","","295","328"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","A","A"]
["","Vermogen","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","","3.85","4.08"]
["","Jaarlijks energieverbruik","","kWu/a","","1578","1704"]