{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FHA50AVEB / RXM50N2V1B","FHA60AVEB / RXM60N2V1B"]
["Koelcapaciteit","Nom.","","kW","5.00","5.70"]
["Koeling","Jaarlijks energieverbruik","","kWu/a","","328"]
["","Vermogen","Pdesign","kW","","5.70"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","","4.71"]
["","Jaarlijks energieverbruik","","kWu/a","","1,704"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","780","867"]
["","EER","","","3.21","3.29"]
["","COP","","","3.35","3.32"]
["","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","C","C"]
["Verwarmingscapaciteit","Nom.","","kW","6.00","7.20"]
["Opmerkingen","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","(3) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(3) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(4) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(4) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Koeling","Energieklasse","","","","A+"]
["","SEER","","","","6.08"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","A"]
["","SCOP/A","","","","3.87"]