{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RZQSG71L3V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L9V1B","FHQ100CAVEB / RZQSG100L9V1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L9V1B","FHQ60CAVEB / FHQ60CAVEB / RZQSG125L9V1B","FHQ125CAVEB / RZQSG125L9V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG125L9V1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQSG125L9V1B","FHQ140CAVEB / RZQSG140L9V1B"]
["Koelcapaciteit","Nom.","","kW","6.8","","9.5","","","12.0","","","13.4"]
["Koeling","SEER","","","5.61","5.10","5.61","5.10","4.80","5.61","4.80","4.80"]
["","Jaarlijks energieverbruik","","kWu/a","424","652","593","652","875","749","875","875"]
["","Vermogen","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energieklasse","","","A+","B","A+","B","B","A+","B","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.60","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.90","3.80","3.91","3.80","3.80","4.01","3.80","3.80"]
["","Energieklasse","","","A","A","A","A","A","A+","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,727","2,800","2,722","2,800","2,800","2,654","2,800","2,800"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","985","","1,480","","","2,075"]
["","EER","","","3.46","","3.21","","","2.89","","","3.01"]
["","COP","","","4.00","","3.61","","","3.62","","","3.41"]
["","Richtlijn Energielabels","Koeling","","A","","A","","","C"]
["","","Verwarming","","A","","A","","","A"]
["Verwarmingscapaciteit","Nom.","","kW","7.5","","10.8","","","13.5","","","15.5"]
["Opmerkingen","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]