{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":23,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ71CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ100CBVEB / RZQG100L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG125L8Y1B","FHQ125CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG125L8Y1B","FHQ60CBVEB / FHQ60CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Koelcapaciteit","Nom.","","kW","6.8","","","","","","9.5","","","","","","","","12.0","","","","13.4"]
["Koeling","SEER","","","6.86","5.10","5.10","6.95","5.10","5.10","6.11","6.11","5.10","5.10","5.10","5.10","5.10","5.10","6.01","6.01","5.10","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","347","467","467","343","467","652","545","545","652","652","652","652","824","824","699","699","824","824"]
["","Vermogen","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Energieklasse","","","A++","B","B","A++","B","B","A++","A++","B","B","B","B","B","B","A+","A+","B","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.60","6.00","6.00","7.60","6.00","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.71","12.71","14.13","14.13","12.71","12.71"]
["","SCOP/A","","","4.32","3.80","3.80","4.32","3.80","3.80","4.61","4.61","3.80","3.80","3.80","3.80","3.80","3.80","4.23","4.23","3.80","3.80"]
["","Energieklasse","","","A+","A","A","A+","A","A","A++","A++","A","A","A","A","A","A","A+","A+","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,463","2,211","2,211","2,463","2,211","4,164","3,432","3,432","4,164","4,164","4,164","4,164","4,683","4,683","4,677","4,677","4,683","4,683"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","890","","","","","","1,245","","","","","","","","1,790","","","","2,025"]
["","EER","","","3.82","","","","","","3.81","","","","","","","","3.35","","","","3.31"]
["","COP","","","4.13","","","","","","4.15","","","","","","","","3.89","","","","3.63"]
["","Richtlijn Energielabels","Koeling","","A","","","","","","A","","","","","","","","A","","","","A"]
["","","Verwarming","","A","","","","","","A","","","","","","","","A","","","","A"]
["Verwarmingscapaciteit","Nom.","","kW","7.5","","","","","","10.8","","","","","","","","13.5","","","","15.5"]
["Opmerkingen","","","","(1) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - SEER en SCOP zijn conform EN 14825","","","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","","","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]