{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Koelcapaciteit","Min.","","kW","1.2"]
["","Max.","","kW","3.8"]
["","Nom.","","kW","3.5"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","6.35"]
["","Gas","Buitendiameter","mm","9.5"]
["","Afvoer","OD","mm","18.0"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Richtlijn Energielabels","Koeling","","B"]
["","","Verwarming","","B"]
["Verwarmingscapaciteit","Nom.","","kW","4.0"]
["","Min.","","kW","1.4"]
["","Max.","","kW","5.0"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - 220V"]
["","","","","(3) - 230V"]
["","","","","(4) - 240V"]
["","","","","(5) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m"]
["","","","","(6) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m"]
["","","","","(7) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]