{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","39","40","41","","46"]
["","","","Middelhoog","dBA","32","33","33","","42"]
["","","","Fluisterstille werking","dBA","19","19","19","","24"]
["","","","Laag","dBA","25","25","25","","33"]
["","Koelen","","Middelhoog","dBA","32","33","33","","39"]
["","","","Fluisterstille werking","dBA","19","19","19","","24"]
["","","","Laag","dBA","25","25","25","","31"]
["","","","Hoog","dBA","39","40","41","","46"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1","","1"]
["","Bedieningshandleiding","","","","1","1","1","","1"]
["","Luchtfilter","","","","2","2","2","","2"]
["","Infrarood-afstandsbediening","","","","1","1","1","","1"]
["","Montageplaat afstandsbediening","","","","1","1","1","","1"]
["","Zakje schroeven","","","","1","1","1","","1"]
["","Schroefdeksel","","","","1","1","1","","1"]
["","AAA drogecelbatterij","","","","2","2","2","","2"]
["","Algemene voorzorgsmaatregelen","","","","1","1","1","","1"]
["Koelmiddel","GWP","","","","675.0","675.0","675.0","","675.0"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50","9.50","","12.70"]
["","Afvoer","","","","18","18","18","","18"]
["Power input","Koelen","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Verwarmen","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Sound power level","Koelen","","","dBA","57","57","60","","60"]
["Afmetingen","Unit","","Breedte","mm","798","798","798","","798"]
["","","","Diepte","mm","189","189","189","","189"]
["","","","Hoogte","mm","295","295","295","","295"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","","Wit"]
["Gewicht","Unit","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Middelhoog","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Laag","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Fluisterstille werking","m³/min","4.5","4.5","4.5","","5.7"]
["","","Koelen","Laag","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Middelhoog","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Hoog","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Fluisterstille werking","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Fase","","","","1~","1~","1~","","1~"]
["","Naam","","","","V1","V1","V1","","V1"]
["","Frequentie","","","Hz","50","50","50","","50"]
["","Spanning","","","V","220-240","220-240","220-240","","220-240"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","","","0.028"]
["","Verwarmen","","Nom.","kW","","","","0.036"]
["Behuizing","Kleur","","","","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","","","","295"]
["","","","Breedte","mm","","","","798"]
["","","","Diepte","mm","","","","189"]
["Gewicht","Unit","","","kg","","","","11.50"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","","","","13.1"]
["","","Koeling","Middelhoog","m³/min","","","","9.8"]
["","","","Laag","m³/min","","","","7.2"]
["","","","Fluisterstille werking","m³/min","","","","4.6"]
["","","Verwarmen","Hoog","m³/min","","","","14.6"]
["","","Verwarming","Middelhoog","m³/min","","","","10.5"]
["","","Verwarmen","Laag","m³/min","","","","7.7"]
["","","","Fluisterstille werking","m³/min","","","","5.2"]
["Geluidsvermogenniveau","Koelen","","","dBA","","","","60"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","","","45"]
["","Koeling","","Middelhoog","dBA","","","","37"]
["","","","Laag","dBA","","","","29"]
["","","","Fluisterstille werking","dBA","","","","21"]
["","Verwarmen","","Hoog","dBA","","","","45"]
["","Verwarming","","Middelhoog","dBA","","","","37"]
["","Verwarmen","","Laag","dBA","","","","29"]
["","","","Fluisterstille werking","dBA","","","","21"]
["Koelmiddel","GWP","","","","","","","675.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","","","6.35"]
["","Gas","","Buitendiameter","mm","","","","12.70"]
["","Drainage","","","","","","","18"]
["Regelsystemen","IR-afstandsbediening","","","","","","","ARC466A58"]
["","Bedrade afstandsbediening","","","","","","","BRC073"]
["Standaard-accessoires","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Luchtfilter","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Voeding","Naam","","","","","","","V1"]
["","Fase","","","","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","","","50"]
["","Spanning","","","V","","","","220-240"]