{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BT / RXA-B"]
[]
[]
[]
[]
["","","","","FTXA42B2V1BT / RXA42B2V1B","FTXA50B2V1BT / RXA50B2V1B","FTXA50B2V1BT / RXA50B5V1B (Archived)"]
["Outdoor unit","","","","RXA42B2V1B","RXA50B2V1B","RXA50B5V1B"]
["Koelcapaciteit","Min.","","kW","1.70","1.70","1.70"]
["","Nom.","","kW","4.20","5.00","5.00"]
["","Max.","","kW","5.00","5.30","5.30"]
["Verwarmingscapaciteit","Min.","","kW","1.70","1.70","1.70"]
["","Nom.","","kW","5.40","5.80","5.80"]
["","Max.","","kW","6.00","6.50","6.50"]
["Nominaal rendement","EER","","","3.99","3.68","3.68"]
["","COP","","","4.12","4.00","4.00"]
["","Jaarlijks energieverbruik","","kWu","526","679","679"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A","A"]
["","","Verwarming","","A","A","A"]
["Koeling","Energieklasse","","","A++","A++","A++"]
["","Vermogen","Pdesign","kW","4.20","5.00","5.00"]
["","SEER","","","7.50","7.33","7.33"]
["","Jaarlijks energieverbruik","","kWu/a","196","239","239"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A++","A++","A++"]
["","Vermogen","Pdesign","kW","3.80","4.00","4.00"]
["","SCOP/A","","","4.60","4.60","4.60"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.56","3.76","3.19"]
["","Jaarlijks energieverbruik","","kWu/a","1150","1217","1218"]