{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-DY / RXA-B9"]
[]
[]
[]
[]
["","","","","FTXA42D2V1BY / RXA42B5V1B9"]
["Koelcapaciteit","Min.","","kW","1.70"]
["","Nom.","","kW","4.20"]
["","Max.","","kW","5.00"]
["Verwarmingscapaciteit","Min.","","kW","1.70"]
["","Nom.","","kW","5.40"]
["","Max.","","kW","6.00"]
["Nominaal rendement","EER","","","3.99"]
["","COP","","","4.12"]
["","Jaarlijks energieverbruik","","kWu","526"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A"]
["","","Verwarming","","A"]
["Koeling","Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","4.20"]
["","SEER","","","7.50"]
["","Jaarlijks energieverbruik","","kWu/a","196"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A++"]
["","Vermogen","Pdesign","kW","3.80"]
["","SCOP/A","","","4.60"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.04"]
["","Jaarlijks energieverbruik","","kWu/a","1156"]
["Bereik van het energierendement","","","","A+++ ~ D"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]