{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":10,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-DY"]
[]
[]
[]
[]
["","","","","","FTXA20D2V1BY","FTXA25D2V1BY","FTXA35D2V1BY","FTXA42D2V1BY","FTXA50D2V1BY"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.020","0.022","0.023","0.028","0.030"]
["","Verwarmen","","Nom.","kW","0.020","0.020","0.220","0.036","0.039"]
["Behuizing","Kleur","","","","Casing: Black, Panel: Dark wood","Casing: Black, Panel: Dark wood","Casing: Black, Panel: Dark wood","Casing: Black, Panel: Dark wood","Casing: Black, Panel: Dark wood"]
["Afmetingen","Unit","","Hoogte","mm","295","295","295","295","295"]
["","","","Breedte","mm","798","798","798","798","798"]
["","","","Diepte","mm","189","189","189","189","189"]
["Gewicht","Unit","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","11.0","11.5","11.9","13.1","13.5"]
["","","Koeling","Middelhoog","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","Laag","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Fluisterstille werking","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Verwarmen","Hoog","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","","Verwarming","Middelhoog","m³/min","8.7","9.0","9.0","10.5","11.1"]
["","","Verwarmen","Laag","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Fluisterstille werking","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Geluidsvermogenniveau","Koelen","","","dBA","57","57","60","60","60"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","39","40","41","45","46"]
["","Koeling","","Middelhoog","dBA","32","33","33","37","39"]
["","","","Laag","dBA","25","25","25","29","31"]
["","","","Fluisterstille werking","dBA","19","19","19","21","24"]
["","Verwarmen","","Hoog","dBA","39","40","41","45","46"]
["","Verwarming","","Middelhoog","dBA","32","33","33","37","42"]
["","Verwarmen","","Laag","dBA","25","25","25","29","33"]
["","","","Fluisterstille werking","dBA","19","19","19","21","24"]
["Koelmiddel","GWP","","","","675.0","675.0","675.0","675.0","675.0"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.50","9.50","9.50","9.50","12.7"]
["","Drainage","","","","18","18","18","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC466A94","ARC466A94","ARC466A94","ARC466A94","ARC466A94"]
["","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Bedieningshandleiding","","","","1","1","1","1","1"]
["","Luchtfilter","","","","2","2","2","2","2"]
["","Infrarood-afstandsbediening","","","","1","1","1","1","1"]
["","Montageplaat afstandsbediening","","","","1","1","1","1","1"]
["","Zakje schroeven","","","","1","1","1","1","1"]
["Bereik van het energierendement","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Voeding","Naam","","","","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240","220-240"]