{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXG-L"]
[]
[]
[]
[]
["","","","","FTXG20LV1BW / RXG20L2V1B","FTXG25LV1BW / RXG25L2V1B","FTXG35LV1BW / RXG35L2V1B","FTXG50LV1BW / RXG50L2V1B"]
["Koelcapaciteit","Min.","","kW","1.3 (2)","1.3 (2)","1.4 (2)","1.7 (2)"]
["","Max.","","kW","2.8 (2)","3.0 (2)","3.8 (2)","5.3 (2)"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","6.35","6.35","6.35","6.35"]
["","Gas","Buitendiameter","mm","9.5","9.5","9.5","12.7"]
["","Afvoer","UD","mm","18","18.0","18.0","18.0"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","250.5","261.5","441","680"]
["","EER","","","4.59 (1)","4.59 (1)","3.97 (1)","3.53 (1)"]
["","COP","","","5.00 (1)","4.42 (1)","4.06 (1)","3.65 (1)"]
["","Richtlijn Energielabels","Koeling","","A","A","A","A"]
["","","Verwarming","","A","A","A","A"]
["Verwarmingscapaciteit","Min.","","kW","1.3 (2)","1.3 (2)","1.4 (2)","1.7 (2)"]
["","Max.","","kW","4.3 (2)","4.5 (2)","5.0 (2)","6.5 (2)"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","(3) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie","(3) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie","(3) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie","(3) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie"]
["","","","","(4) - 220V","(4) - 220V","(4) - 220V","(4) - 220V"]
["","","","","(5) - 230V","(5) - 230V","(5) - 230V","(5) - 230V"]
["","","","","(6) - 240V","(6) - 240V","(6) - 240V","(6) - 240V"]