{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-M"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40M2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40M2V1B"]
["Koelcapaciteit","Nom.","","kW","4.00","4.00"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","482","467"]
["","EER","","","4.15","4.28"]
["","COP","","","3.95","4.32"]
["","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","A"]
["Verwarmingscapaciteit","Nom.","","kW","4.60","4.60"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]