{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Koelcapaciteit","Nom.","","kW","4.00","","5.20","4.00","4.00","6.00"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","467","","593","471","457","787"]
["","EER","","","4.28","","4.38","4.25","4.38","3.81"]
["","COP","","","4.32","","4.42","4.05","4.04","3.88"]
["","Richtlijn Energielabels","Koeling","","A","","A","A","A","A"]
["","","Verwarming","","A","","A","A","A","A"]
["Verwarmingscapaciteit","Nom.","","kW","4.60","","6.80","6.80","6.50","7.80"]
["Koelcapaciteit","Nom.","","kW","","4.00"]
["Verwarmingscapaciteit","Nom.","","kW","","4.60"]
["Nominaal rendement","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Jaarlijks energieverbruik","","kWh","","482"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","","A"]
["","","Verwarming","","","A"]
["Koeling","Energieklasse","","","","A++"]
["","Vermogen","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Jaarlijks energieverbruik","","kWu/a","","164"]
["Verwarming (gematigd klimaat)","Energieklasse","","","","A+"]
["","Vermogen","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","","3.58"]
["","Jaarlijks energieverbruik","","kWu/a","","1632"]
["Opmerkingen","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]