{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":11,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N"]
[]
[]
[]
[]
["","","","","","FTXP35N5V1B","FTXP50N2V1B","FTXP60N2V1B","FTXP71N2V1B","FTXP20N5V1B (Archived)","FTXP25N5V1B (Archived)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.032","0.029","0.032","0.032","0.019","0.02"]
["","Verwarmen","","Nom.","kW","0.032","0.032","0.035","0.035","0.023","0.023"]
["Behuizing","Kleur","","","","Wit","Wit","Wit","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","286","295","295","295","286","286"]
["","","","Breedte","mm","770","990","990","990","770","770"]
["","","","Diepte","mm","225","263","263","263","225","225"]
["Gewicht","Unit","","","kg","9","13.5","13.5","13.5","8.5","8.5"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","11.5","16.3","16.8","16.8","9.5","9.7"]
["","","Koeling","Middelhoog","m³/min","8.3","14","14.4","14.4","7.4","7.7"]
["","","","Laag","m³/min","6.3","11.5","11.8","11.8","5.6","5.8"]
["","","","Fluisterstille werking","m³/min","4.5","8.3","9.2","10.1","4.2","4.2"]
["","","Verwarmen","Hoog","m³/min","11.5","17.3","17.9","17.9","10.4","10.4"]
["","","Verwarming","Middelhoog","m³/min","9","14.4","15.3","15.3","8.1","8.1"]
["","","Verwarmen","Laag","m³/min","7","11.8","12.4","12.4","6.2","6.4"]
["","","","Fluisterstille werking","m³/min","5.3","10.4","11","11","5.2","5.2"]
["Geluidsvermogenniveau","Koelen","","","dBA","58","59","60","62","55","55"]
["","Verwarmen","","","dBA","58","61","62","62","55","55"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","43","43","45","46","39","40"]
["","Koeling","","Middelhoog","dBA","34","39","41","42","33","33"]
["","","","Laag","dBA","27","34","36","37","25","26"]
["","","","Fluisterstille werking","dBA","20","27","30","32","19","19"]
["","Verwarmen","","Hoog","dBA","40","42","44","45","39","40"]
["","Verwarming","","Middelhoog","dBA","35","38","40","41","34","34"]
["","Verwarmen","","Laag","dBA","29","33","35","36","28","28"]
["","","","Fluisterstille werking","dBA","21","30","32","33","21","21"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6","6.4","6.4","6.4","6","6"]
["","Gas","","Buitendiameter","mm","9.5","12.7","12.7","12.7","9.5","9.5"]
["","Drainage","","","","18","18","18","18","18","18"]
["Regelsystemen","Infrared remote control","","","","ARC480A78","ARC480A53","ARC480A53","ARC480A53"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","General safety precautions","","","","1","","","","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Voeding","Naam","","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standaard-accessoires","WLAN adapter kit","","","","","1","1","1"]
["Regelsystemen","IR-afstandsbediening","","","","","","","","ARC480A78","ARC480A78"]
["Opmerkingen","","","","","","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)"]
["","","","","","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]