{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","40","","","","","","45"]
["","","","Fluisterstille werking","dBA","19","","","","","","22"]
["","","","Laag","dBA","27","","","","","","33"]
["","Koelen","","Fluisterstille werking","dBA","19","","","","","","21"]
["","","","Laag","dBA","24","","","","","","33"]
["","","","Hoog","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Koelen","","Nom.","dBA","32","","","","","","39"]
["Standaard-accessoires","Montagehandleiding","","","","1","","","","","","1"]
["","Bedieningshandleiding","","","","1","","","","","","1"]
["","Draadloze afstandsbediening","","","","1","","","","","","1"]
["","Batterijen","","","","2","","","","","","2"]
["","Afstandsbedieningshouder","","","","1","","","","","","1"]
["","Montageplaat","","","","1","","","","","","1"]
["","Montageschroeven binnenunit","","","","2","","","","","","2"]
["","Fotokatalytisch luchtzuiveringsfilter uit titaniumapatiet","","","","2","","","","","","2"]
["Control systems","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","","","","","","6.35"]
["","Gas","","Buitendiameter","mm","9.5","","","","","","9.5"]
["","Afvoer","","","","18","","","","","","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Verwarmen","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Geluidsniveau","Koelen","","","dBA","58","","","","","","59"]
["","Verwarmen","","","dBA","58","","","","","","59"]
["Afmetingen","Unit","","Breedte","mm","780","","","","","","900"]
["","","","Diepte","mm","215","","","","","","215"]
["","","","Hoogte","mm","289","","","","","","298"]
["Casing","Colour","","","","Wit","","","","","","Wit"]
["Gewicht","Unit","","","kg","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Frequentie","","","Hz","50","","","","","","50"]
["","Naam","","","","V1","","","","","","V1"]
["","Spanning","","","V","220-240","","","","","","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Verwarmen","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Behuizing","Kleur","","","","","Wit","Wit","Wit","Wit","Wit","","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","","215","289","215","298","215","","215","298","215"]
["","","","Breedte","mm","","780","780","780","900","900","","900","900","900"]
["","","","Diepte","mm","","289","215","289","215","298","","298","215","298"]
["Gewicht","Unit","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","Koeling","Middelhoog","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Laag","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Fluisterstille werking","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Verwarmen","Hoog","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","Verwarming","Middelhoog","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Verwarmen","Laag","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Fluisterstille werking","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Geluidsvermogenniveau","Koelen","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Verwarmen","","","dBA","","58","58","58","59","59","","59","60","60"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","40","41","41","45","45","","45","46","46"]
["","Koeling","","Middelhoog","dBA","","32","33","33","","37","","39","","40"]
["","","","Laag","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Fluisterstille werking","dBA","","19","19","19","19","19","","21","23","23"]
["","Verwarmen","","Hoog","dBA","","40","41","41","45","45","","45","47","47"]
["","Verwarming","","Middelhoog","dBA","","34","34","34","","39","","39","","40"]
["","Verwarmen","","Laag","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Fluisterstille werking","dBA","","19","19","19","19","19","","22","24","24"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Drainage","","","","","18","18","18","18","18","","18","18","18"]
["Control systems","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standaard-accessoires","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Voeding","Naam","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fase","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Spanning","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilator","Luchtdebiet","Koelen","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilator","Luchtdebiet","Verwarmen","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Geluidsdrukniveau","Verwarmen","","Nom.","dBA","","","34","","39","","","","40"]
["Regelsystemen","IR-afstandsbediening","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standaard-accessoires","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Opmerkingen","","","","","","","","","","","(4) - 240V"]