{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / RZASG100M7V1B","FUA125AVEB9 / RZASG125M7V1B","FUA71AVEB / RZASG71M2V1B","FUA71AVEB9 / RZASG71M2V1B","FUA71AVEB9 / FUA71AVEB9 / RZASG140M7V1B"]
["Koelcapaciteit","Nom.","","kW","","","6.80 (1)","6.80 (1)"]
["Koeling","SEER","","","","","6.16","6.16"]
["","Jaarlijks energieverbruik","","kWu/a","","","386","386"]
["","Vermogen","Pdesign","kW","","","6.80","6.80"]
["","Energieklasse","","","","","A++","A++"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","","","4.50","4.50"]
["","SCOP/A","","","","","3.90","3.90"]
["","Energieklasse","","","","","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","","","1,615","1,615"]
["Verwarmingscapaciteit","Nom.","","kW","","","7.50 (2)","7.50 (2)"]
["Opmerkingen","","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Koelcapaciteit","Nom.","","kW","9.5","12.1","","","13.4"]
["Verwarmingscapaciteit","Nom.","","kW","10.8","13.5","","","15.5"]
["Koeling","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","9.5","12.1","","","13.4"]
["","SEER","","","5.83","5.49","","","8.56"]
["","Jaarlijks energieverbruik","","kWu/a","570","1322","","","939"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+"]
["","Vermogen","Pdesign","kW","6","6","","","7.80"]
["","SCOP/A","","","4.01","3.84","","","5.00"]
["","Jaarlijks energieverbruik","","kWu/a","2095","2188","","","2185"]