{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","","","","41","46","47"]
["","","","Middelhoog","dBA","","","","38","42","43"]
["","","","Laag","dBA","","","","35","39","40"]
["","Koelen","","Middelhoog","dBA","","","","38","42","43"]
["","","","Laag","dBA","","","","35","39","40"]
["","","","Hoog","dBA","","","","41","46","47"]
["Standaard-accessoires","Bedieningshandleiding","","","","","","","1","1","1"]
["","Montagehandleiding","","","","","","","1","1","1"]
["","Afvoerslang","","","","","","","1","1","1"]
["","Thermische isolatiebuis","","","","","","","3","3","3"]
["","Kabelbinders","","","","","","","10","10","10"]
["","Slangband","","","","","","","1","1","1"]
["","Afdichtingsmateriaal","","","","","","","4","4","4"]
["","Sluitring bevestigingsplaat","","","","","","","1","1","1"]
["","Afvoerkoppeling","","","","","","","1","1","1"]
["","Non-woven textiel","","","","","","","1","1","1"]
["","Sluitring","","","","","","","8","8","8"]
["","Montageschroef voor afvoerslang","","","","","","","5","5","5"]
["Control systems","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Koelcapaciteit","Totale capaciteit","","Nom.","kW","","","","","","12.1"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","","","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","","","","15.9","15.9","15.9"]
["","Drain","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Geluidsvermogenniveau","Koelen","","","dBA","","","","59","64","65"]
["","Verwarmen","","","dBA","","","","59","64"]
["Afmetingen","Unit","","Breedte","mm","","","","950","950","950"]
["","","","Diepte","mm","","","","950","950","950"]
["","","","Hoogte","mm","","","","198","198","198"]
["Casing","Material","","","","","","","Hars","Hars","Hars"]
["","Colour","","","","","","","Zuiver wit","Zuiver wit","Zuiver wit"]
["Gewicht","Unit","","","kg","","","","25.0","26.0","26"]
["Ventilator","Luchtdebiet","Verwarmen","Hoog","m³/min","","","","23.0","31.0","32.5"]
["","","","Middelhoog","m³/min","","","","19.5","25.5","26.5"]
["","","","Laag","m³/min","","","","16.0","20.0","20.5"]
["","","Koelen","Laag","m³/min","","","","16.0","20.0","20.5"]
["","","","Middelhoog","m³/min","","","","19.5","25.5","26.5"]
["","","","Hoog","m³/min","","","","23.0","31.0","32.5"]
["Afvoerhoogte","mm","","","","","","","600","600","600"]
["Verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","","","","","","13.5"]
["Behuizing","Kleur","","","","Zuiver wit","Zuiver wit","Zuiver wit"]
["","Materiaal","","","","Hars","Hars","Hars"]
["Afmetingen","Unit","","Hoogte","mm","198","198","198"]
["","","","Breedte","mm","950","950","950"]
["","","","Diepte","mm","950","950","950"]
["Gewicht","Unit","","","kg","25.0","26.0","26.0"]
["Ventilator","Luchtdebiet","Koelen","Hoog","m³/min","23.0","31.0","32.5"]
["","","Koeling","Middelhoog","m³/min","19.5","25.5","26.5"]
["","","","Laag","m³/min","16.0","20.0","20.5"]
["","","Verwarmen","Hoog","m³/min","23.0","31.0","32.5"]
["","","Verwarming","Middelhoog","m³/min","19.5","25.5","26.5"]
["","","Verwarmen","Laag","m³/min","16.0","20.0","20.5"]
["Geluidsvermogenniveau","Koelen","","","dBA","59","64","65"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","41","46","47"]
["","Koeling","","Middelhoog","dBA","38","42","43"]
["","","","Laag","dBA","35","39","40"]
["","Verwarmen","","Hoog","dBA","41","46","47"]
["","Verwarming","","Middelhoog","dBA","38","42","43"]
["","Verwarmen","","Laag","dBA","35","39","40"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.9","15.9","15.9"]
["","Drainage","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Afvoerhoogte","mm","","","","600","600","600"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Koelcapaciteit","Totale capaciteit","","Nom.","kW","","","12.10"]
["Verwarmingscapaciteit","Totaalvermogen","","Nom.","kW","","","13.5"]