{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUQ100CVEB / RZQG71L8Y1B","FUQ71CVEB / RZQG71L8Y1B","FUQ100CVEB / RZQG100L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG100L8Y1B","FUQ71CVEB / FUQ71CVEB / RZQG125L8Y1B","FUQ125CVEB / RZQG125L8Y1B"]
["Koelcapaciteit","Nom.","","kW","","6.8","9.5","","","12.0"]
["Koeling","SEER","","","6.50","6.42","6.11","5.10","5.10","5.61"]
["","Jaarlijks energieverbruik","","kWu/a","367","371","545","652","824","749"]
["","Vermogen","Pdesign","kW","6.80","6.80","9.5","9.50","12.00","12"]
["","Energieklasse","","","A++","A++","A++","B","B","A+"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","7.60","7.60","11.3","11.30","12.71","14.13"]
["","SCOP/A","","","4.20","4.20","4.5","3.80","3.80","4.44"]
["","Energieklasse","","","A+","A+","A+","A","A","A+"]
["","Jaarlijks energieverbruik","","kWu/a","2,534","2,534","3,516","4,164","4,683","4,456"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","","840","1,230","","","1,770"]
["","EER","","","","4.05","3.86","","","3.39"]
["","COP","","","","4.08","3.95","","","3.42"]
["","Richtlijn Energielabels","Koeling","","","A","A","","","A"]
["","","Verwarming","","","A","A","","","B"]
["Verwarmingscapaciteit","Nom.","","kW","","7.5","10.8","","","13.5"]
["Opmerkingen","","","","","(1) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","(2) - SEER en SCOP zijn conform EN 14825","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]