{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["","","Laag","dBA","38","44","46","48"]
["","Koelen","Laag","dBA","38","44","46","48"]
["","","Hoog","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["Standaard-accessoires","Bedieningshandleiding","","","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding"]
["","Montagehandleiding","","","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding"]
["","Montagebeugel","","","Montagebeugel","Montagebeugel","Montagebeugel","Montagebeugel"]
["","Rubberbescherming voor opening","","","Rubberbescherming voor opening","Rubberbescherming voor opening","Rubberbescherming voor opening","Rubberbescherming voor opening"]
["","Huls","","","Huls","Huls","Huls","Huls"]
["","Isolatie voor fitting","","","Isolatie voor fitting","Isolatie voor fitting","Isolatie voor fitting","Isolatie voor fitting"]
["","Deksel","","","Deksel","Deksel","Deksel","Deksel"]
["","Klemmen","","","Klemmen","Klemmen","Klemmen","Klemmen"]
["","Schroeven","","","Schroeven","Schroeven","Schroeven","Schroeven"]
["","Montagepatroon","","","Montagepatroon","Montagepatroon","Montagepatroon","Montagepatroon"]
["","Dauwbestendig materiaal","","","Dauwbestendig materiaal","Dauwbestendig materiaal","Dauwbestendig materiaal","Dauwbestendig materiaal"]
["","Bedrading afstandsbediening","","","Bedrading afstandsbediening","Bedrading afstandsbediening","Bedrading afstandsbediening","Bedrading afstandsbediening"]
["Regelsystemen","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Piping connections","Vloeistof","Buitendiameter","mm","9.52","9.52","9.52","9.52"]
["","Gas","Buitendiameter","mm","15.9","15.9","15.9","15.9"]
["","Afvoer","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Opgenomen vermogen","Koelen","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Verwarmen","Nom.","kW","0.117","0.238","0.238","0.276"]
["Geluidsvermogenniveau","Koelen","","dBA","55","62","63","65"]
["","Verwarmen","","dBA","55","62","63","65"]
["Afmetingen","Unit","Breedte","mm","600","600","600","600"]
["","","Diepte","mm","270","350","350","350"]
["","","Hoogte","mm","1,850","1,850","1,850","1,850"]
["Behuizing","Colour","","","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit"]
["Gewicht","Unit","","kg","39","47","47","47"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequentie","","Hz","50/60","50/60","50/60","50/60"]
["","Spanning","","V","220-240/220","220-240/220","220-240/220","220-240/220"]