{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-M"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25M2V1B","FVXG35K2V1B / RXLG35M2V1B"]
["Outdoor unit","","","","RXLG25M","RXLG35M"]
["Koelcapaciteit","Min.","","kW","1.2","1.4"]
["","Nom.","","kW","2.5","3.5"]
["","Max.","","kW","5.1","5.6"]
["Verwarmingscapaciteit","Min.","","kW","1.0","1.1"]
["","Nom.","","kW","4.5","5.6"]
["","Max.","","kW","6.5, 3.5","7.0, 4.0"]
["Nominaal rendement","EER","","","3.52","3.43"]
["","COP","","","3.88","3.61"]
["","Jaarlijks energieverbruik","","kWu","355","510"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","A"]
["Leidingaansluitingen","Afvoer","UD","mm","18","18"]
["","Gas","Buitendiameter","mm","9.5","9.5"]
["","Vloeistof","Buitendiameter","mm","6.35","6.35"]
["Koeling","Energieklasse","","","A++","A++"]
["","Vermogen","Pdesign","kW","2.50","3.50"]
["","SEER","","","6.99","6.59"]
["","Jaarlijks energieverbruik","","kWu/a","131","186"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+","A+"]
["","Vermogen","Pdesign","kW","3.00","3.40"]
["","SCOP/A","","","4.25","4.01"]
["","Jaarlijks energieverbruik","","kWu/a","988","1187"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Voor minimaal verwarmingsvermogen, ventilator van binnenunit instellen op SL-stand","(6) - Voor minimaal verwarmingsvermogen, ventilator van binnenunit instellen op SL-stand"]
["","","","","(7) - Maximaal verwarmingsvermogen bij buitentemperatuur van -15°C","(7) - Maximaal verwarmingsvermogen bij buitentemperatuur van -15°C"]