{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":12,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMA-A"]
[]
[]
[]
[]
["","","","","","FXMA50A5VEB","FXMA63A5VEB","FXMA80A5VEB","FXMA100A5VEB","FXMA125A5VEB","FXMA200AXVMB","FXMA250AXVMB"]
["Geluidsdrukniveau","Verwarmen","","Bij hoge ventilatorsnelheid","dBA","","","","","","48.0"]
["","","","Bij lage ventilatorsnelheid","dBA","","","","","","45.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","","","","","","46.5"]
["","Koelen","","Bij lage ventilatorsnelheid","dBA","","","","","","45.0"]
["","","","Bij hoge ventilatorsnelheid","dBA","","","","","","48.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","","","","","","46.5"]
["Standaard-accessoires","Montage- en bedieningshandleiding","","","","","","","","","1"]
["","Draadklem","","","","","","","","","1"]
["","Veerring","","","","","","","","","2"]
["","Zeskantschroef","","","","","","","","","2"]
["","Vlakke sluitring","","","","","","","","","8"]
["","Zeskantschroef met sluitring","","","","","","","","","49"]
["","Gasaansluitleiding","","","","","","","","","1"]
["","Algemene voorzorgsmaatregelen","","","","","","","","","1"]
["Koelmiddel","GWP","","","","","","","","","675"]
["","Type","","","","","","","","","R-32"]
["Opgenomen vermogen - 50Hz","Koelen","","Bij hoge ventilatorsnelheid","kW","","","","","","0.54"]
["","Verwarmen","","Bij hoge ventilatorsnelheid","kW","","","","","","0.54"]
["Koelcapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","","","","","","22.4"]
["","Nom.","","","kW","","","","","","22.4"]
["Piping connections","Vloeistof","","Buitendiameter","mm","","","","","","9.5"]
["","","","Type","","","","","","","Flareverbinding"]
["","Gas","","Buitendiameter","mm","","","","","","19.1"]
["","","","Type","","","","","","","Flens"]
["","Afvoer","","","","","","","","","BSP1"]
["Geluidsvermogenniveau","Koelen","","Bij hoge ventilatorsnelheid","dBA","","","","","","75.0"]
["Afmetingen","Unit","","Breedte","mm","","","","","","1,490"]
["","","","Diepte","mm","","","","","","1,100"]
["","","","Hoogte","mm","","","","","","470"]
["Behuizing","Materiaal","","","","","","","","","Gegalvaniseerde staalplaat"]
["","Colour","","","","","","","","","Ongelakt"]
["Gewicht","Unit","","","kg","","","","","","105"]
["Ventilator","Externe statische druk - 50Hz","","Hoog","Pa","","","","","","250"]
["","","","Laag","Pa","","","","","","50"]
["","Externe statische druk - 60Hz","","Hoog","Pa","","","","","","250"]
["","","","Laag","Pa","","","","","","50"]
["","Luchtdebiet - 50Hz","Koelen","Bij hoge ventilatorsnelheid","m³/min","","","","","","62"]
["","","","Bij lage ventilatorsnelheid","m³/min","","","","","","41"]
["Verwarmingscapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","","","","","","25.0"]
["","Nom.","","","kW","","","","","","25.0"]
["Stroom - 50Hz","Maximaal zekeringamperage (MFA)","","","A","","","","","","6"]
["Power supply","Phase","","","","","","","","","1~"]
["","Naam","","","","","","","","","VM"]
["","Frequentie","","","Hz","","","","","","50/60"]
["","Spanning","","","V","","","","","","220-240/220-230"]
["Koelvermogen","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","5.6","7.1","9.0","11.2","14.0","","28.0"]
["Verwarmingscapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","6.3","8.0","10.0","12.5","16.0","","31.5"]
["Opgenomen vermogen - 50Hz","Koelen","","Bij hoge ventilatorsnelheid","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["","Verwarmen","","Bij hoge ventilatorsnelheid","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["Afmetingen","Unit","","Hoogte","mm","300","300","300","300","300","","470"]
["","","","Breedte","mm","1,000","1,000","1,000","1,400","1,400","","1,490"]
["","","","Diepte","mm","700","700","700","700","700","","1,100"]
["Gewicht","Unit","","","kg","35","35","35","46","46","","115"]
["Behuizing","Kleur","","","","Ongelakt","Ongelakt","Ongelakt","Ongelakt","Ongelakt","","Ongelakt"]
["","Materiaal","","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","","Gegalvaniseerde staalplaat"]
["Vereiste plafondruimte >-=-mm","mm","","","","350","350","350","350","350"]
["Ventilator","Luchtdebiet - 50Hz","Koelen","Bij hoge ventilatorsnelheid","m³/min","18.0","19.5","25.0","32.0","36.0","","74"]
["","","","Bij lage ventilatorsnelheid","m³/min","15.0","16.0","20.0","23.0","26.0","","52"]
["","Externe statische druk - 50Hz","","Hoog","Pa","200","200","200","200","200","","250"]
["","Externe statische druk - 60Hz","","Hoog","Pa","200","200","200","200","200","","250"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","","R-32"]
["","GWP","","","","675","675","675","675","675","","675"]
["Geluidsniveau","Koelen","","Bij hoge ventilatorsnelheid","dBA","61.0","64.0","67.0","65.0","70.0","","76.0"]
["Geluidsdrukniveau","Koelen","","Bij hoge ventilatorsnelheid","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","Bij lage ventilatorsnelheid","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["","Verwarmen","","Bij hoge ventilatorsnelheid","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","Bij lage ventilatorsnelheid","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["Leidingaansluitingen","Vloeistof","","Type","","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","","Flareverbinding"]
["","","","Buitendiameter","mm","6.35","6.35","6.35","9.52","9.52","","9.5"]
["","Gas","","Type","","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","Flareverbinding","","Flens"]
["","","","Buitendiameter","mm","12.7","12.7","12.7","15.9","15.9","","19.1"]
["","Drainage","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","","BSP1"]
["Luchtfilter","Type","","","","Kunstharsnet","Kunstharsnet","Kunstharsnet","Kunstharsnet","Kunstharsnet"]
["Standaard-accessoires","Washer for hanger bracket","","","","8","8","8","8","8"]
["","Drain hose","","","","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","","1"]
["","Insulation for fitting","","","","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1"]
["","Screws","","","","16","16","16","16","16"]
["","Sealing pad","","","","3","3","3","3","3"]
["Voeding","Naam","","","","VE","VE","VE","VE","VE","","VM"]
["","Fase","","","","1~","1~","1~","1~","1~","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50/60","50/60","50/60","50/60","50/60","","50/60"]
["","Spanning","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","","220-240/220-230"]
["Stroom: 50 Hz","Maximaal zekeringamperage (MFA)","","","A","6","6","6","6","6","","6"]
["Ventilator","Externe statische druk - 50Hz","","Laag","Pa","","","","","","","50"]
["","Externe statische druk - 60Hz","","Laag","Pa","","","","","","","50"]
["Standaard-accessoires","General safety precautions","","","","","","","","","","1"]
["","Wire clamp material","","","","","","","","","","1"]
["","Spring washer","","","","","","","","","","2"]
["","Hexagon head screw","","","","","","","","","","2"]
["","Plain washer","","","","","","","","","","8"]
["","Hexagon head screw with washer","","","","","","","","","","49"]
["","Gas connection pipe","","","","","","","","","","1"]