{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-A"]
[]
[]
[]
[]
["","","","","","FXMQ200AXVMB","FXMQ250AXVMB"]
["Koelvermogen","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","22.4","28.0"]
["Verwarmingscapaciteit","Totaalvermogen","","Bij hoge ventilatorsnelheid","kW","25.0","31.5"]
["Opgenomen vermogen - 50Hz","Koelen","","Bij hoge ventilatorsnelheid","kW","0.54","0.65"]
["","Verwarmen","","Bij hoge ventilatorsnelheid","kW","0.54","0.65"]
["Afmetingen","Unit","","Hoogte","mm","470","470"]
["","","","Breedte","mm","1490","1490"]
["","","","Diepte","mm","1100","1100"]
["Gewicht","Unit","","","kg","105","115"]
["Behuizing","Kleur","","","","Ongelakt","Ongelakt"]
["","Materiaal","","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["Ventilator","Luchtdebiet - 50Hz","Koelen","Bij hoge ventilatorsnelheid","m³/min","62","74"]
["","","","Bij lage ventilatorsnelheid","m³/min","41","52"]
["","Externe statische druk - 50Hz","","Hoog","Pa","250","250"]
["","","","Laag","Pa","50","50"]
["","Externe statische druk - 60Hz","","Hoog","Pa","250","250"]
["","","","Laag","Pa","50","50"]
["Koelmiddel","Type","","","","R-410A","R-410A"]
["","GWP","","","","2087.5","2087.5"]
["Geluidsniveau","Koelen","","Bij hoge ventilatorsnelheid","dBA","75.0","76.0"]
["Geluidsdrukniveau","Koelen","","Bij hoge ventilatorsnelheid","dBA","48.0","48.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","46.5","46.5"]
["","","","Bij lage ventilatorsnelheid","dBA","45.0","45.0"]
["","Verwarmen","","Bij hoge ventilatorsnelheid","dBA","48.0","48.0"]
["","","","Bij gemiddelde ventilatorsnelheid","dBA","46.5","46.5"]
["","","","Bij lage ventilatorsnelheid","dBA","45.0","45.0"]
["Leidingaansluitingen","Vloeistof","","Type","","Flareverbinding","Flareverbinding"]
["","","","Buitendiameter","mm","9.5","9.5"]
["","Gas","","Type","","Flens","Flens"]
["","","","Buitendiameter","mm","19.1","22.2"]
["","Drainage","","","","BSP1","BSP1"]
["Standaard-accessoires","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","1","1"]
["","Spring washer","","","","2","2"]
["","Hexagon head screw","","","","2","2"]
["","Plain washer","","","","8","8"]
["","Hexagon head screw with washer","","","","49","49"]
["","Gas connection pipe","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["Voeding","Naam","","","","VM","VM"]
["","Fase","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50/60","50/60"]
["","Spanning","","","V","220-240/220-230","220-240/220-230"]
["Stroom: 50 Hz","Maximaal zekeringamperage (MFA)","","","A","6","6"]